i-PRO WJ-NX400 NETWORK DISK RECORDER
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 19 DIGITAL VIDEO RECORDERS AND ANALOG RECORDING DEVICES

This specification is intended for use by the design/construction professional and any user of i-PRO Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormat^TM 2014 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	i-PRO Sensing Solutions Co., Ltd

B.	Provide Video Surveillance Camera from single source manufacturer 

2.2	i-PRO WJ-NX400 NETWORK DISK RECORDER

A.	GENERAL CHARACTERISTICS
1.	The Network Disk Recorder (NDR) shall be an all-in-one recording solution for IP video surveillance system of up to 128 network cameras.

2.	The NDR shall store H.264 video data and H.265 video data.

3.	The NDR shall have the capability of up to 640 Mbps total throughput. (Recording throughput : 384 Mbps, Output throughput : 256 Mbps)

4.	The NDR shall offer 324TB (54 x 6TB HDD) of gross storage capacity with five optional Hard Disk Extension units. 

5.	The NDR shall offer hardware RAID 1, RAID 5 and RAID 6 data protection internally and with optional Hard Disk Extension units. 

6.	The NDR shall offer VMD search function which can search the moving of the selected specific area.

7.	The NDR shall record two streams per camera.

8.	The NDR shall manage HDDs for reduce a HDD operation time by managing HDD status and controlling a HDD motor

9.	The NDR shall offer TURBO-RAID for quick RAID recovery without sacrificing recording bandwidth and performance

10.	The NDR shall manage redundant fail-over using 2nd recorder to enable mission-critical recording by KMS registration

11.	The NDR shall backup important data to NAS devices by KMS registration

12.	The NDR shall monitor on multiscreen mode including corridor mode screen layout.

13.	The NDR shall offer displaying videos on the main and sub monitors connected to HDMI interface.

14.	The NDR shall set up to two camera group for different saving period of recorded image.

15.	The NDR shall offer the operation and configuration functions to the cameras and NDR from the main monitor connected to HDMI interface and mouse. 

16.	The NDR shall store an encrypted stream and shall display encrypted streams/videos by decrypting.

17.	The NDR shall realize optional SSL / TLS communication with CA certificate. 

18.	The NDR shall offer remote and mobile monitoring on a PC, smartphone and tablet.

19.	The NDR shall conform to the ONVIF standard. 

B.	NETWORK DISK RECORDER
1.	Inputs			Up to 128 network cameras support 
2.	Protocols			i-PRO series Network cameras Onvif NVT conformant  
camera and encoder camera
C.	FUNCTIONS
1.	Display
a.	Local display		HDMI / 4K (Main monitor), Full HD (Sub monitor), 
analog composite video
b.	Multiscreen Display	Main monitor: 1, 2, 3, 4, 5, 6, 7, 9, 12, 16, 24, 32,64
Sub monitor: 1, 4,16, 32
c.	Camera control	Panning, Tilting, Zoom, Focus, Brightness, Preset position call
and program (up to 256), Auto mode, Click centering, Wheel
zoom, Zoom reset, Auto Back Focus, Aux, Wiper(for WV-
SUD638)
d.	System Setup	Setup page in English, French, Italian, Spanish, German, Russian,
Portuguese, Thai, Simplified Chinese, Traditional Chinese, Japanese

2.	Recording
a.	Image format		H.265, H.264, MJPEG
b.	Frame rate		Up to 60 fps per stream (Depending on the Camera)
c.	Recording rate	384 Mbps or less
d.	Audio		G.711 for Onvif, G.726 (ADPCM) 32 kbps, AAC-LC
e.	Recording Mode	Schedule, Event (Pre/Sub stream), Emergency
f.	Alarm Source	32 terminal inputs, 
128 camera alarms ( TCP alarm notification),  
128 command alarms
g.	Event Action		Alarm recording, e-mail notification, Alarm message, 
Camera positioning, Terminal output,  TCP alarm notification output, Buzzer, Indicator

3.	Search and Playback
a.	Search mode	Date and time (Calendar), Timeline, Video Motion Detection
(VMD) , log list, Thumbnail
b.	Playback control	Play, Reverse Play, Pause, Stop, Fast Forward, Fast Reverse, 
Previous Record, Next Record, Previous Image, Next Image, Go to Date, Go to Last (Jumps to 30 seconds before the record end)
Time-saving playback
c.	De-warping		1 de-warped playback of fisheye view video

4.	Remote and mobile monitoring
a.	Remote monitoring	Web browser: Microsoft IE
WV-ASM300 i-PRO management software, SYSTEM 970 
b.	Mobile monitoring	i-PRO Mobile APP software on iOS and Android
c.	Re-encoding		2 clients

5.	Management
a.	User registration	Up to 32 users
b.	Simultaneous users	16 or less
c.	Authentication	User authentication (ID and Password), Host authentication
d.	User level		Administrator and customizable 3-level user authentication
e.	Quick setup		Set-up wizard with Automatic camera detection
f.	Central management	WV-ASM300 i-PRO management software, SYSTEM 970

D.	STORAGE
1.	HDD slot
a.	Internal		9 HDD slots
b.	External unit		45 HDD slots with 5 WJ-HXE400 Hard Disk External Units
2.	HDD type			3.5 inch SATA HDD
3.	RAID(Hardware RAID)	RAID 1,5, 6

E.	INTERFACE
1.	Indicator/Button
a.	Indicator		LCD, Status indicator: ALARM, ERROR, OPERATE, REC, 
  HDD(status), HDD(access)
b.	Button		Display content switching button
2.	Connections
a.	Network		2x 10BASE-T/100BASE-TX/1000BASE-TX(RJ-45)
b.	Video		2x HDMI, 1x BNC
c.	Audio		1x RCA pin jack
d.	External Storage	5x Expansion connectors for Hard Disk Extension Unit
e.	Alarm/Control	56pin Terminal blocks
(2x 16pin Terminal blocks, 2x 12pin Terminal blocks)
f.	Mouse		2x mouse connection port USB2.0
g.	Copy port		2x USB 3.0 port
h.	Power cord	
WJ-NX400K		1x Power cord
WJ-NX400K/G	2x Power cord
3.	Slots
a.	HDD			9x HDD slots 

F.	ELECTRICAL
1.	Power Source		
a.	WJ-NX400K		120 V AC, 60 Hz
b.	WJ-NX400K/G  	220-240 V AC, 50/60 Hz
2.	Power Consumption	
a.	WJ-NX400 		Approx. 125W (with 6 TB HDD x9)
b.	WJ-HXE400		Approx. 85W(170VA)
WJ-HXE400/G	Approx. 85W(175VA)

G.	MECHANICAL
1.	Dimensions 		430 mm (W) x 132 mm (H) x 413 mm
                                           (Depth from Rack Mount Bracket is 400 mm)
16-15/16 inches (W) x 5-3/16 inches (H) x 16-1/4 inches (D)
                                                               (Depth from Rack Mount Bracket is 15-3/4")
(Excluding rubber feet and projections)
2.	Weight
a.	Without HDD		11.5 kg {25.4 lbs}
b.	With 9 HDDs		20.0 kg {44.1 lbs} 

H.	ENVIRONMENTAL
1.	Ambient Operating Temperature
				+5 °C ~ +45 °C (41 °F ~ 113 °F)
2.	Ambient Operating Humidity
				 5 % ~ 90 % (without condensation)

I.	APPROVALS
1.	Safety / EMC Standard	
a.	WJ-NX400K		UL (UL60065), FCC (Part15 Class A), 
C-UL (CAN/CSA C22.2 No.60065), DOC (ICES003 Class A)
b.	WJ-NX400K/G	CE (EN60065, EN55032 Class B, EN55024), EAC

J.	SOFTWARE OPTIONS
1.	WJ-NXE40 / WJ-NXE40W Additional Camera Kit(Two licenses for 32 cameras)
2.	WJ-NXS32 / WJ-NXS32W Secure optional license for 32 channel
3.	WJ-NXS16 / WJ-NXS16W Secure optional license for 16 channel
4.	WJ-NXS04 / WJ-NXS04W Secure optional license for 4 channel
5.	WJ-NXS01 / WJ-NXS01W Secure optional license for 1 channel

K.	HARDWARE OPTION
1.	WJ-HXE400 Hard Disk Extension Unit(AC120V)
2.	WJ-HXE400/G Hard Disk Extension Unit(AC220V-240V)