i-PRO WJ-NX310KG NETWORK DISK RECORDER
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 19 DIGITAL VIDEO RECORDERS AND ANALOG RECORDING DEVICES

This specification is intended for use by the design/construction professional and any user of i-PRO Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormat^TM 2014 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 
     Warranty | i-PRO Products

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	i-PRO Co., Ltd

B.	Provide Video Surveillance Camera from single source manufacturer 

2.2	i-PRO WJ-NX310KG NETWORK DISK RECORDER

A.	GENERAL CHARACTERISTICS
1.	The Network Disk Recorder (NDR) shall be an all-in-one recording solution for IP video surveillance system of up to 32 network cameras.

2.	The NDR shall store H.264 video data and H.265 video data.

3.	The NDR shall have the capability of up to 512 Mbps total throughput. (Recording throughput : 256 Mbps, Output throughput : 256 Mbps)

4.	The NDR shall offer hardware RAID 1 data protection internally and with optional Hard Disk Extension units. 

5.	The NDR shall offer VMD search function which can search the moving of the selected specific area.

6.	The NDR shall manage HDDs for reduce a HDD operation time by managing HDD status and controlling a HDD motor

7.	The NDR shall offer TURBO-RAID for quick RAID recovery without sacrificing recording bandwidth and performance.

8.	The NDR shall manage redundant fail-over using 2nd recorder to enable mission-critical recording by KMS registration.

9.	The NDR shall backup important data to NAS devices by KMS registration

10.	The NDR shall monitor on multiscreen mode including corridor mode screen layout.

11.	The NDR shall offer displaying videos on the main and sub monitors connected to HDMI interface.

12.	The NDR shall set up to two camera group for different saving period of recorded image.

13.	The NDR shall offer the operation and configuration functions to the cameras and NDR from the main monitor connected to HDMI interface and mouse. 

14.	The NDR shall store an encrypted stream and shall display encrypted streams/videos by decrypting.

15.	The NDR shall realize optional SSL / TLS communication with CA certificate. 

16.	The NDR shall offer remote and mobile monitoring on a PC, smartphone and tablet.

17.	The NDR shall conform to the ONVIF standard. 

B.	NETWORK DISK RECORDER
1.	Inputs			Up to 32 network cameras support 
2.	Protocols			i-PRO series Network cameras Onvif NVT conformant  
camera and encoder camera
C.	FUNCTIONS
1.	Display
a.	Local display		HDMI / 4K (Main monitor), Full HD (Sub monitor), 
analog composite video
b.	Multiscreen Display	Main monitor: 1, 2, 3, 4, 5, 6, 7, 9, 12, 16, 24, 32
Sub monitor: 1, 4,16
c.	Camera control	Panning, Tilting, Zoom, Focus, Brightness, Preset position call
and program (up to 256), Auto mode, Click centering, Wheel
zoom, Zoom reset, Auto Back Focus, Aux, Wiper (for WV-
SUD638), Active ClearSight
d.	System Setup	Setup page in English, French, Italian, Spanish, German,
Portuguese, Thai, Vietnamese, Simplified Chinese, Traditional Chinese, Japanese

2.	Recording
a.	Image format		H.265(HEVC), H.264, JPEG
b.	Frame rate		Up to 60 fps per stream (Depending on the Camera)
c.	Recording rate	256 Mbps or less
d.	Audio		G.711 for Onvif, AAC-LC
e.	Recording Mode	Event, Schedule, Emergency, Pre-event recording
f.	Alarm Source	9x terminal inputs, 
32x camera alarms (TCP alarm notification),  
128x command alarms
g.	Event Action		Alarm recording, e-mail notification, Alarm message, 
Camera positioning, Terminal output, TCP alarm notification, HTTP alarm notification, Buzzer, Indicator

3.	Search and Playback
a.	Search mode	Search criteria: Time date, Playback by designating a timeline,
Thumbnail
b.	Playback control	Play, Reverse Play, Pause, Stop, Fast Forward, Fast Reverse, 
Previous Record, Next Record, Previous Image, Next Image, Go to Date, Go to Last (Jumps to 30 seconds before the record end)
Time-saving playback
c.	De-warping		Only 1ch display mode, Display : 1-Screen PTZ / 4-Screen PTZ

4.	Remote and mobile monitoring
a.	Remote monitoring	Web browser: Microsoft IE
b.	Mobile monitoring	i-PRO Mobile APP software on iOS and Android
c.	Re-encoding		2 clients

5.	Management
a.	User registration	Up to 32 users
b.	Simultaneous users	16 or less
c.	Authentication	User authentication (ID and Password), Host authentication
d.	User level		Administrator and customizable 3-level user authentication
e.	Quick setup		Set-up wizard with Automatic camera detection

D.	STORAGE
1.	HDD slot
a.	Internal		4 HDD slots
2.	HDD type			3.5 inch SATA HDD
3.	RAID(Hardware RAID)	RAID 1

E.	INTERFACE
1.	Indicator/Button
a.	Indicator		LCD, Status indicator: ALARM, ERROR, OPERATE, REC, 
  HDD(status), HDD(access)
b.	Button		Display content switching button
2.	Connections
a.	Network		2x 10BASE-T/100BASE-TX/1000BASE-TX(RJ-45)
b.		Monitor (HDMI) Connector
	                         [Main monitor]
HDMI 4K UHD(3840x2160p)/30Hz, 4K UHD(3840x2160p)/25Hz,
1920x1080p /60Hz, 1920x1080p /50Hz,
[Sub monitor]
HDMI 4K UHD(3840x2160p)/30Hz, 4K UHD(3840x2160p)/25Hz,
1920x1080p /60Hz, 1920x1080p /50Hz,
c.	Mouse		x1 USB2.0 conformant port in front side
DC5V/500mA (with over current limitation function)
                       
d.	USB Storage             Front: USB 3.0/USB 2.0 stick, 
USB 3.0/USB 2.0 HDD (self-powered device only)
                                                                Rear: USB 3.0/USB 2.0 stick, 
USB 3.0/USB 2.0 HDD (self-powered device only), 
USB 3.0/USB 2.0 SSD 
(both of self and bus-powered devices)
3.	Slots
a.	HDD			4x HDD slots 

F.	ELECTRICAL
a.	Power Source	AC100-240 V(±10%), 50/60 Hz
b.	Power Consumption	95W, 100VA

G.	MECHANICAL
1.	Dimensions 		420 mm (W) x 88 mm (H) x 370 mm
                                           16-17/32 inches (W) x 3-15/32 inches (H) x 14-9/16 inches (D)
                                                              
2.	Weight
a.	Without HDD		7.5 kg {16.56 lbs}
H.	ENVIRONMENTAL
1.	Ambient Operating Temperature
				+5 °C ~ +40 °C (41 °F ~ 104 °F)
2.	Ambient Operating Humidity
				 5 % ~ 90 % (without condensation)

I.	APPROVALS
1.	Safety / EMC Standard	DEMKO (IEC62368-1), CE/UKCA (EN55032/EN55035)
J.	Extension Software
1.	Camera Extension Kit        WJ-NXE32W (16ch→24ch→32ch) WJ-NXE33W (16ch→32ch)
2.	Secure Communication Kit  WJ-NXS01W, WJ-NXS04W, WJ-NXS16W,WJ-NXS32W