i-PRO WV-S25700-V2LG FIXED NETWORK CAMERA
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SONSORS

This specification is intended for use by the design/construction professional and any user of i-PRO Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormat^TM 2014 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	i-PRO Co., Ltd

B.	Provide Video Surveillance Camera from single source manufacturer 

2.2	i-PRO WV-S25700-V2LG FIXED NETWORK CAMERA

A.	GENERAL CHARACTERISTICS
1.	The Fixed Camera shall deliver H.265 stream and H.264 stream. 

2.	The Fixed Camera shall produce a resolution of 3840x2160 pixels at up to 30 fps with a 16:9 aspect ratio. 

3.	The Fixed Camera shall utilize an approximate 1/1.8 type high sensitivity CMOS image sensor. 

4.	The Fixed Camera shall feature a 132dB wide dynamic range based on Enhanced Super Dynamic and Adaptive Black Stretch technology (ABS). 

5.	The Fixed Camera shall produce a color image with a minimum illumination of 0.06 lux and a monochrome image with 0.03 lux at F1.5, shutter speed of 1/30s and AGC 11. 

6.	The Fixed Camera shall offer a built-in IR illumination to produce a clear monochrome image in zero lux conditions with 50m (164feet) irradiation distance.

7.	The Fixed Camera shall generate multiple simultaneous video streams of up to four (4) H.265 (Main profile) or H.264 (High profile) streams and JPEG streams.

8.	The Fixed cameras should be equipped with the improved intelligent auto mode to monitors the dynamics and movement of important subject’s scenes and to capture license plates and human faces more clearly.

9.	The fixed camera should be equipped with the improved smart coding with GOP control (including frame control), and it monitors the movement of important subject’s scenes to reduce bit rate for longer recording and reduce network load.  

10.	The Fixed Camera shall be equipped with corridor mode enables the capture of a more
vertically-oriented area than the normal format would allow.
                                                                                         
11.	The Fixed Camera shall produce encrypted stream.

12.	The Fixed Camera shall realize SSL / TLS communication with CA certificate. 

13.	A user shall be able to view video on a PC using a browser.

14.	A user shall be able to view video on a smartphone and tablet using viewer software for iPhone and Android.

15.	The Fixed Camera shall offer Video Motion Detection (VMD) with four (4) programmable detection areas, 15 steps sensitivity level and 10 steps detection size.

16.	The Fixed Camera shall offer intelligent Video Motion Detection (i-VMD) with four (4) detection modes as intruder detection, loitering detection, direction detection, 
and cross line detection.

17.	The Fixed Camera shall have Fog compensation function.

18.	The Fixed Camera shall have High light compensation (HLC) function.

19.	The Fixed Camera shall have Super Chroma Compensation (SCC) which realizes a better color reproducibility in the low illumination.

20.	The Fixed Camera shall provide up to eight (8) areas of electronic privacy masking. 

21.	The Fixed Camera shall offer the prioritized stream control which transmits a video stream to a specified client PC or recorder preferentially. 

22.	The Fixed Camera shall have a SD memory card slot that supports SD, SDHC and SDXC memory card for local storage. 

23.	The Fixed Camera shall offer full-duplex bi-directional audio communication capability between the camera and monitoring site. 

24.	The Fixed Camera shall have three (3) alarm sources of terminal input, VMD, and command alarm that activate the processes such as SDXC/ SDHC/SD memory recording, E-mail notification, HTTP alarm notification, Indication on browser and TCP alarm notification output.

25.	The Fixed Camera shall conform to the ONVIF standard. 

B.	CAMERA
1.	Image Sensor		1/1.8 type CMOS image sensor
2.	Effective Pixels                  Approx. 4K pixels
3.	Scanning Mode		Progressive
4.	Minimum Illumination
a.	Color		0.06 lux (F1.5, Maximum shutter: Off (1/30s), AGC: 11)
b.	B/W			0.0 lux (with IR LED on)
0.03 lux (F1.5, Maximum shutter: Off (1/30s), AGC: 11)
5.	Day & Night		IR Cut filter Removal
6.	Dynamic Range		132 dB typ. (Super Dynamic: On)
7.	Built-in IR illumination
a.	Irradiation distance	Approx. 50m (164feet:50IRE)

C.	Lens
1.	Focal Length		4.3 ~ 8.6mm (5/32 ~ 11/32 inches)
2.	Max. Aperture Ratio	1 : 1.5 (WIDE) ~ 1 : 2.4 (TELE)
3.	Angular Field of View
a.	16:9 mode		H: 52° (TELE) - 101° (WIDE)
V: 29° (TELE) -   55° (WIDE)

4.	Adjusting Angle		Horizontal : -194 to +166°,Vertical : -30 to +85°,Yaw : ±100°
5.	Focus adjustment		Auto focus
6.	Optical Zoom Ratio           2.0x 

D.	VIDEO
1.	Compression Format	H.265, H.264, JPEG
2.	Image Resolution
a.	16:9 aspect ratio
3840 x 2160 / 2560 x 1440 / 1920 x 1080 / 1280 x 720 / 640 x 360 / 
320 x 180
3.	H.265 / H.264
a.	Transmission Mode	Constant bit rate / VBR, Frame rate / Best effort
b.	Frame Rate		1 / 3 / 5 / 7.5 / 10 / 12 / 15 / 20 / 30 fps (30fps)
c.	                                  1 / 3.1 / 4.2 / 6.25 / 8.3 / 12.5 / 20 / 25 fps (25fps)
                                           *Super Dynamic: On, Level: 30 or more, 15fps

d.	Bit Rate/Client	64 / 128 / 256 / 384 / 512 / 768 / 1024 / 1536 / 2048 / 3072 / 
4096 / 6144 / 8192 / 10240 / 12288 / 14336 / 16384 / 20480 / 
24576 kbps / --FREE ENTRY--
e.	Image Quality	
i.	Constant bit rate	Low (Motion priority) / Normal / Fine (Image quality priority)
ii.	Frame rate            Low (Motion priority) / Normal / Fine (Image quality priority)
iii.	Best effort	Low (Motion priority) / Normal / Fine (Image quality priority)
iv.	VBR		10 steps
f.	Transmission type	Unicast port (AUTO)/ Unicast port (MANUAL)/ Multicast
4.	JPEG
a.	Image quality	10 steps 
b.	Transmission type	Pull, Push
5.	Smart Coding
a.	GOP(Group of picture) control
On (Frame rate control)* / On (Advanced)* / On (Low) / On (Mid) / Off 
*On (Frame rate control) and On (Advanced) are only available with H.265.
b.	Auto VIQS     	On / Off

E.	Audio
a.	Audio Compression	G.726 (ADPCM) 32kbps / 16kbps, G.711 64kbps, 
AAC-LC 128 / 96 / 64 kbps
b.	Audio Mode		OFF / Mic(Line) input / Audio output / Interactive (Half duplex) /
Interactive (Full duplex)

F.	OPERATION
1.	Super Dynamic		On / Off
The level can be set in the range of 0 to 31.
2.	Intelligent Auto 		On / Off
3.	Adaptive Black Stretch	The level can be set in the range of 0 to 255.
4.	Fog compensation	On / Off (Only when Intelligent Auto is off.)

5.	Black light compensation
High light compensation	BLC (Black light compensation) / HLC (High light compensation) /
Off 
(Only when Super dynamic and Intelligent Auto is off)
6.	AGC			The level can be set in the range of 0 to 11.
7.	Shutter Speed		1/10000 to 1/30 s (30fps/15fps mode)
                                          1/10000 to 1/25 s (25fps/12.5fps mode)
8.	Day & Night		Off/ On (IR Light Off)/ On (IR Light On)/ Auto1 (IR Light Off)/
Auto2 (IR Light On)/ Auto3 (SCC)
9.	Digital Noise Reduction	The level can be set in the range of 0 to 255.
10.	Video Motion Detection	On / Off, 4 areas, Sensitivity:15 steps, Detection size:10 steps
11.	Intelligent Video Motion Detection
5 detection modes (Intruder Detection, Loitering Detection,
Direction Detection, Object Detection, Cross Line Detection)
12.	Privacy Zone		On / Off, Up to 8 zones
13.	Camera Title (OSD)	Up to 20 characters
14.	Digital Zoom		2.0x – 6.0x (when resolution is 1280 x 720)

G.	NETWORK
1.	Network Interface		10Base-T / 100Base-TX, RJ-45 connector
2.	IP			IPv6, IPv4
3.	Supported Protocols
a.	IPv6			TCP/IP, UDP/IP, HTTP, HTTPS, RTP, SMTP, DNS, NTP,
SNMP, DHCPv6, MLD, ICMP, ARP, IEEE 802.1X, DiffServ, LLDP, SRTP, SSL/TLS, SFTP, MQTT
b.	IPv4			TCP/IP, UDP/IP, HTTP, HTTPS, RTSP, RTP, RTP/RTCP,
SMTP, DHCP, DNS, DDNS, NTP, SNMP, UPnP, IGMP, ICMP,
ARP, IEEE 802.1X, DiffServ, LLDP, SRTP, SSL/TLS, SFTP, MQTT
4.	Max. User access		Up to 14 users
5.	Mobile Terminal Compatibility
iPad, iPhone, Android^TM mobile terminals

H.	INTERFACE
1.	Monitor Output		VBS : 1.0 V [p-p] / 75 ohm, NTSC / PAL composite, Pin jack
2.	Microphone input / Line input
				ø3.5 mm stereo mini jack
3.	Audio Output		ø3.5 mm stereo mini jack (monaural output) 
4.	External I/O Terminals	ALARM IN 1 (Alarm input 1/ Black & white input/
Auto time adjustment input) (x1)
 ALARM IN 2 (Alarm input 2/ ALARM OUT) (x1)
ALARM IN 3 (Alarm input 3/ AUX OUT) (x1)
5.	SD memory card slot	1 slot, SD/SDHC/SDXC

I.	ELECTRICAL
1.	Power Source		DC 12V/1.0A, PoE (DC48V/240mA, Class 0)
2.	Power Consumption	Approx. 12.0W (DC 12V), Approx. 11.5W (PoE)

J.	SAFETY / EMC
1.	Safety			UL (UL62368-1), C-UL (CSA C22.2 No.62368-1), CE, 
				IEC62368-1
2.	EMC 			FCC (Part15 Class A), ICES003 Class A, EN55032 Class A, 
				EN55035

K.	MECHANICAL
1.	Dimensions 		Φ154 mm x 105 mm (H)  
{Φ6-1/316 inches x 4-1/8 inches (H)} 
2.	Weight			Approx. 1.1 kg (2.43lbs.)
3.	Construction material
a.	Main body		Aluminum die cast
b.	Front cover		Polycarbonate resin
4.	Finish
a.	Main body		i-PRO white
b.	Dome cover		Smoke

L.	ENVIRONMENTAL
1.	Vandal Resistance	Compliant with IEC 62262 IK10
2.	Operating Temperature	-10 °C ~ +60 °C (-40 °F ~ 140 °F)
 (Power On range: –30 °C to +60 °C {–22 °F to +140 °F})
3.	Operating Humidity	 10 % ~ 100 % (no condensation)