i-PRO WV-S6532LN PTZ DOME NETWORK CAMERA
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SONSORS

This specification is intended for use by the design/construction professional and any user of Panasonic Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormat^TM 2014 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	i-PRO Sensing Solutions Co., Ltd.

B.	Provide Video Surveillance Camera from single source manufacturer 

2.2	i-PRO WV-S6532LN PTZ NETWORK CAMERA

A.	GENERAL CHARACTERISTICS
1.	The PTZ Camera shall deliver H.265 stream and H.264 stream. 

2.	The PTZ Camera shall produce a resolution of 1920 x 1080 pixels(Full HD)
 at up to 60 fps with a 16:9 aspect ratio. 

3.	The PTZ Camera shall produce a resolution of 2048 x 1536 pixels at 30fps with a 4:3 aspect ratio. 

4.	The PTZ Camera shall utilize an approximate 1/2.8-inch type high sensitivity CMOS image sensor.  

5.	The PTZ Camera shall be equipped with 22 times optical zoom. 

6.	The PTZ Camera shall feature an intelligent image stabilization to capture stable images even when installing on the plenty-vibration place. 

7.	The PTZ Camera shall feature a 144dB wide dynamic range based on Enhanced Super Dynamic 

8.	The PTZ Camera shall produce a color image with a minimum illumination of 0.015 lux and a monochrome image with 0.006 lux at F1.6, shutter speed of 1/30s and AGC 11.

9.	The PTZ Camera shall offer a built-in IR illumination to produce a clear monochrome image in zero lux conditions with 100m (330 feet) irradiation distance.

10.	The PTZ Camera shall be equipped with a special coated cover for increasing the operational utility of outdoor cameras in rain weather.

11.	The PTZ Camera shall transmit up to four(4) video streams  simultaneously which can be selected to H.265 (Main profile) or H.264 (High profile) or JPEG(can be selected up  to two(2) video streams only).

12.	The PTZ Camera shall be equipped with intelligent auto mode, the technology for shooting license plate and person’s face more clearly.

13.	The PTZ Camera shall be equipped with GOP control of bitrate reducing technology which five control modes included frame rate control for longer recording and less storage.

14.	The PTZ Camera shall produce encrypted stream.

15.	The PTZ Camera shall realize SSL / TLS communication with CA certificate. 

16.	A user shall be able to view video on a PC using a browser.

17.	A user shall be able to view video on a smartphone and tablet using viewer software for iPhone and Android.

18.	The PTZ Camera shall offer Video Motion Detection (VMD) with four (4) programmable detection areas, 15 steps sensitivity level and 10 steps detection size.

19.	The Fixed Dome Camera shall offer intelligent Video Motion Detection (i-VMD) with six (6) detection modes as intruder detection, loitering detection, scene change detection,
object detection and cross line detection

20.	The PTZ Camera shall offer an optional intelligent VMD (i-VMD) function which provides intruder detection, loitering detection, direction detection, scene change detection, object detection and cross line detection.

21.	The PTZ Camera shall have Fog compensation function.

22.	The PTZ Camera shall have High light compensation (HLC) function.

23.	The PTZ Camera shall provide up to thirty-two (32) areas of electronic privacy masking. 

24.	The PTZ Camera shall offer the prioritized stream control which transmits a video stream to a specified client PC or recorder preferentially. 

25.	The PTZ Camera shall have an SD memory card slot that supports SD, SDHC and SDXC memory card for local storage. 

26.	The PTZ Camera shall offer full-duplex bi-directional audio communication capability between the camera and monitoring site. 

27.	The PTZ Camera shall have three (3) alarm sources of terminal input, VMD, command alarm, audio detection alarm and auto track alarm that activate the processes such as SDXC/ SDHC/SD memory recording, E-mail notification, HTTP alarm notification, Indication on browser, FTP image transfer and  TCP alarm notification output.

28.	The PTZ Camera shall conform to the ONVIF profile S and profile G. 

B.	CAMERA
1.	Image Sensor		1/2.8-inch type CMOS image sensor
2.	Scanning Mode		Progressive
3.	Minimum Illumination
a.	Color		0.015 lux (F1.6, Maximum shutter: Off(1/30s), AGC: 11)
b.	B/W			0.0 lux (IR LED is on)
0.001 lux (F1.6, Maximum shutter: Off(1/30s), AGC: 11)
4.	Day & Night		IR Cut filter Removal
5.	Dynamic Range		144 dB typ. (Super Dynamic: On)

C.	Lens
1.	Focal Length		4.25 ~ 95mm (5/32 inches – 3-3/4 inches)
2.	Max. Aperture Ratio	1 : 1.6 (WIDE) ~ 1 : 3.7 (TELE)
3.	Angular Field of View
a.	16:9 aspect ratio	H:  3.4° (TELE) -  66° (WIDE)
V:  2.0° (TELE) -  39° (WIDE)
b.	4:3 aspect ratio	H:  2.6° (TELE) -  51° (WIDE)
V:  2.0° (TELE) -  39° (WIDE)

D.	VIDEO
1.	Compression Format	H.265, H.264, JPEG
2.	Image Resolution
a.	16:9 aspect ratio (2 mega pixel mode)
1920 x 1080 / 1280 x 720 / 640 x 360 / 320 x 180 (30/60fps)
b.	4:3 aspect ratio (3 mega pixel mode)
2048 x 1536 / 1280 x 960 / 800 x 600 / 640 x 480 / 400 x 300 / 320 x 240 (30fps)
3.	H.265 / H.264
a.	Transmission Mode	Constant bit rate / VBR, Frame rate / Best effort
b.	Frame Rate		1 / 3 / 5 / 7.5 / 10 / 12 / 15 / 20 / 30 / 60 fps
c.	Bit Rate/Client	64 / 128 / 256 / 384 / 512 / 768 / 1,024 / 1,536 / 2,048 / 3,072 / 
4,096 / 6,144 / 8,192 / 10,240 / 12,288 / 14,336 / 16,384 / 20,480 / 24,576 / 30,720 / 40,960 kbps
d.	Image Quality	
i.	Constant bit rate	Motion priority / Normal / Quality priority
ii.	Best effort	Motion priority / Normal / Quality priority
iii.	VBR		10 steps
e.	Transmission type	Unicast, Multicast
4.	JPEG
a.	Image quality	10 steps 
b.	Transmission type	Pull, Push

E.	Audio
a.	Audio Compression	G.726 (ADPCM) 32kbps / 16kbps, 
G.711 64kbps, 
AAC-LC 64kbps / 96kbps / 128kbps
b.	Audio Mode		OFF / Mic input / Audio output / Interactive (Half duplex) /
Interactive (Full duplex)

F.	OPERATION
1.	Super Dynamic		On / Off
*The Super Dynamic function is automatically set to off(60fps).
The level can be set in the range of 0 to 31.
2.	Intelligent Auto 		On / Off
3.	Adaptive Black Stretch	The level can be set in the range of 0 to 255.
4.	Fog compensation	On / Off (Only when Intelligent Auto is off.)
5.	Black light compensation
High light compensation	BLC (Black light compensation) / HLC (High light compensation) /
Off 
(Only when Super dynamic and Intelligent Auto is off)
6.	Shutter speed		Off(1/30) to 1/10000
*1/30 Fix to 2/100 Fix is available during 30 fps mode only.
*2/120 Fix is available during 60 fps mode only.
7.	Day & Night		On / Off / Auto1 (Normal) / Auto2 (IR Light) 
8.	Digital Noise Reduction	The level can be set in the range of 0 to 255.
9.	Video Motion Detection	On / Off, 4 areas, Sensitivity:15 steps, Detection size:10 steps

10.	Intelligent Video Motion Detection
                                           6 detection modes(Intruder Detection, Loitering Detection,
Direction Detection, Scene Change Detection)
Object Detection, Cross Line Detection 
11.	Intelligent Zoom Stabilizer On / Off (available only in the 30 fps mode)
                                           *Auto track, Smart Facial Coding, i-VMD, can not be used
 at the same time.
12.	Privacy Zone		On / Off, Up to 8 zones
13.	Camera Title (OSD)	Up to 20 characters
14.	Zoom Ratio		22x
15.	Digital zoom		16x
16.	Panning Range		360-degrees endless
17.	Panning Speed	
a.	Manual		Approx. 0.065°/s to 150°/s, Up to 256 steps 
(Depending on the controller)
b.	Preset		Up to approx. 300°/s
18.	Tilting Range		-30° to 210°
19.	Tilting Speed
a.	Manual		Approx. 0.065°/s to 150°/s, Up to 256 steps 
b.	Preset		Up to approx. 300°/s

G.	NETWORK
1.	Network Interface		10Base-T / 100Base-TX, RJ-45 connector
2.	IP			IPv6, IPv4
3.	Supported Protocols
a.	IPv6			TCP/IP, UDP/IP, HTTP, HTTPS, RTP, FTP, SMTP, DNS, NTP,
SNMP, DHCPv6, MLD, ICMP, ARP, DiffServ, IEEE 802.1x
b.	IPv4			TCP/IP, UDP/IP, HTTP, HTTPS, RTSP, RTP, RTP/RTCP, FTP,
SMTP, DHCP, DNS, DDNS, NTP, SNMP, UPnP, IGMP, ICMP,
ARP, DiffServ, IEEE 802.1x
4.	Max. User access		Up to 14 users
5.	Mobile Terminal Compatibility
iPad, iPhone(OS 4.2.1 or later）, Android^TM mobile terminals

H.	INTERFACE
1.	Monitor Output		VBS : 1.0 V [p-p] / 75 ohm, NTSC / PAL composite
2.	Microphone input / Line input
				ø3.5 mm stereo mini jack (monaural input)
3.	Audio Output		ø3.5 mm stereo mini jack (monaural output) 
4.	External I/O Terminals	ALARM IN 1 (DAY/NIGHT IN), ALARM IN 2 (ALARM OUT),
ALARM IN 3 (AUX OUT)
5.	SD memory card slot	1 slot, SD/SDHC/SDXC

I.	ELECTRICAL
1.	Power Source		AC24V/3.4A,  PoE+ DC54V/470 mA (Class 4 device), 
Tested PoE Injector(60W, DC54V/1.0A)
2.	Power Consumption	Approx. 55W (AC 24V), Approx. 25W (PoE+)
Approx. 50W (Tested PoE injector)

J.	SAFTEY / EMC
1.	Safety			UL (UL60950-1), c-UL (CSA C22.2 No.60950-1), 
EN60950-1 
2.	EMC			FCC (Part15 Class A), ICES003 Class A, EN55032 Class A, 
				EN55024

K.	MECHANICAL
1.	Dimensions(D x H)	ø249 mm × 500 mm (ø9-13/16 inches × 19-11/16 inches)
2.	Weight			Approx. 8.2 kg {18.10 lbs}

3.	Construction Material	
a.	Main Body 		Aluminum die cast
b.	Front Panel		Polycarbonate resin  
  (with ClearSight coating (rain wash coating)),                  
4.	Finish		
a.	Main body		Fine silver
b.	Front Panel		Clear

L.	ENVIRONMENTAL
1.	Ingress Resistance	IP66, IEC60529 measuring standard compatible, 
Type 4X(UL50E), NEMA 4X compliant
2.	Vandal Resistance	IEC 62262 IK10
3.	Operating Temperature	-40 °C ~ +60 °C (-40 °F ~ 140 °F) 
(AC 24 V/ Tested PoE injector (60 W))
-30 °C ~ +60 °C (-22 °F ~ 140 °F, PoE+)
{Power On range: –30 °C to +60 °C (–22 °F to +140 °F)}
4.	Operating Humidity	 10 % ~ 100 % (without condensation)