4.1 Alarm type
•
Terminal alarm: When connecting an alarm device such as a sensor to the alarm input terminal of the camera, the alarm action will be performed when the connected alarm device is activated.
•
VMD alarm: When motion is detected in the set VMD area, the alarm action will be performed.
*VMD stands for “Video Motion Detection”.
•
Command alarm: When a Panasonic alarm protocol is received from the connected device via a network, the alarm action will be performed.
•
Audio detection alarm: When the configured audio detection level is exceeded, the alarm action will be performed.