Section 6 Display the log list
The history of various logs will be displayed in list form.
•
Alarm log: Logs of the alarm occurrences such as time and date of the alarm occurrences, the image recording period and the alarm type will be displayed.
•
Manual/Schedule log: Logs filed when images have been recorded manually or during the period of the schedule, and the image recording period will be displayed.
•
FTP trans. error log: Logs filed when the FTP periodic image transmission function has failed will be displayed.
1.
Display the “Live” page.
2.
Click the [List/Play] button.
→
The log list will be displayed in a newly opened window (log list window).
IMPORTANT
•
Only a single user can operate the log list window. Other users cannot access the log list window.
Time
Displays the time period of the data recorded on the SD memory card.
Recording stream
Select the recording stream that you want to display logs for.
•
Stream 1: The logs recorded by “Recording stream 1” on the [SD memory card] tab will be displayed.
•
Stream 2: The logs recorded by “Recording stream 2” on the [SD memory card] tab will be displayed.
Event
Select a log type to display on the log list.
•
All: All logs will be displayed.
•
Select: Only the logs of the selected log type will be displayed.
–
Alarm log: The log when an alarm is detected will be displayed.
–
Manual/Schedule log: Manual and Schedule logs will be displayed.
–
FTP trans. error log: Logs filed when the FTP periodic image transmission function has failed will be displayed.
•
Default: All
Note
•
When “Stream 1” is selected for “Recording stream” and either “JPEG(1)”, “JPEG(2)”, or “JPEG(3)” is selected for “Stream 1”, the FTP trans. error log will be displayed.
Recording time
Configure the time period of logs displayed on the log list.
•
From: Configure the starting period of logs displayed on the log list.
–
First recording: Displays from the first log recorded on the SD memory card.
–
Today: Displays the logs recorded today.
–
Yesterday: Displays the logs recorded from yesterday to the present day.
–
Last 7 days: Displays the logs recorded from 6 days ago to the present day.
–
Last 30 days: Displays the logs recorded from 29 days ago to the present day.
–
Date/time: Displays the logs recorded from the entered date and time on “Date/time” box.
•
To: Configure the ending period of logs displayed on the log list when “First recording” or “Date/time” is selected for “From”.
–
Last recording: Displays until the last log recorded on the SD memory card.
–
Date/time: Displays the logs recorded until the entered date and time on “Date/time” box.
[Search] button
Searches for logs according to the conditions specified in “Event” and “Recording time”.
The search result will be displayed on the log list.
Log list
Displays the log search results.
You can play back recorded data by clicking on the time or duration of the recorded data displayed under [Time] and [Duration].
•
[Top] button: Click this button to display the log listed at the top.
•
[Prev. page] button: Click this button to display the previous page of the log list.
•
[Next page] button: Click this button to display the next page of the log list.
•
[Last] button: Click this button to display the log listed at the bottom.
•
[Time & date]: Time and date when each log has been recorded will be displayed.
Note
•
When “Off” is selected for “Time display format”, the alarm occurrence times are displayed in 24 hour time format.
•
The recording timing of logs is as follows.
–
Alarm log: Alarm occurrence time and date will be filed as a log.
–
Manual/Schedule log: Time and date when recording of images onto the SD memory card started manually or during the period of the schedule will be filed as a log. When images are recorded sequentially, if “JPEG” is selected for “Recording format”, logs will be filed on the hour every hour (12:00, 1:00, 2:00, etc.). If “H.264” is selected for “Recording format”, logs will be filed every hour from the time when recording starts. However, depending on the photographic subject and the setting used, logs may be filed in periods of over an hour.
–
FTP trans. error log: Logs will be filed every one hour.
•
[Duration]: Displays the period of time that the data has been recorded on the SD memory card.
Note
•
The difference between the recording end time and recording start time of the image is calculated by rounding off to the nearest tenth of a second. For this reason, when only 1 JPEG image is saved, 00:00:00 is displayed for the duration.
•
[Event]: The event type will be displayed.
–
MN/SC: Log by “Manual/Schedule”
–
TRM1: Alarm by alarm input to Terminal 1
–
TRM2: Alarm by alarm input to Terminal 2
–
TRM3: Alarm by alarm input to Terminal 3
–
VMD: Alarm by VMD alarm
–
COM: Alarm by command alarm
–
AUD: Alarm by audio detection alarm
–
FTP: Logs saved from FTP periodic image transmission errors
•
[SD memory card]: Available capacity and the original capacity of the SD memory card will be displayed.
•
[Delete] button: Click this button to delete the currently displayed log list. When using the SD memory card, images associated with the log list will also be deleted.
IMPORTANT
•
If there are too many recorded data files, it may take time to delete all of them. (When the total size is 1 GB, it may require about 1 hour.) Formatting the SD memory card can shorten the time to delete all the data.
•
In the process of the deletion, “Alarm” and “Manual/Schedule” cannot be operated.
•
Do not turn off the power of the camera until the deletion is complete. When the power of the camera is turned off in the process of the deletion, some images may remain on the SD memory card. In this case, click the [Delete] button on the same log list window used to delete the logs.
•
[Download] button: Click this button to download all logs of the selected log list onto the PC.
Note
•
The following settings may be required.
Open Internet Explorer, click [Tools] → [Internet Options] → [Security] → [Trusted Sites] → [Sites]. Register the camera address on [Website] of the displayed trusted windows.
After registration, close the web browser, and then access the camera again.
•
Up to 50,000 logs will be downloaded to the SD memory card. When more than 50,000 logs are filed, the older logs will be overwritten by the newer logs. In this case, the oldest log is the first to be overwritten.
•
[Close] button: Click this button to close the log list window.