11.9 Configure the VIQS area
The VIQS area is specified by following the steps below.
1.
Drag the mouse on the screen to specify the area (up to 8 areas).
→
The specified area is set to area “1(White)”, and the outline is displayed.
The areas are set in the area number order from number 1. The color next to the area number show the color of the corresponding outline.
2.
Configure the difference level in the image quality between specified areas and non-specified areas. The greater the difference level, the more the image quality of the non-specified area is reduced. This makes it possible to moderate the image data size.
3.
Select On/Off to activate/deactivate a distributed image of “H.264(1)”, “H.264(2)”, “H.264(3)”, or “H.264(4)”.
4.
Click the [Set] button.
→
This unit is updated with the setting contents. Click the [Delete] button corresponding to the area to be deleted.
5.
Click the [Confirm] button.
→
The image (“H.264(1)”, “H.264(2)”, “H.264(3)”, or “H.264(4)”) that the [Confirm] button was pressed for is displayed. When a window is newly opened and about 3 seconds pass, the currently outputted bit rate can be confirmed with the configured VIQS.
IMPORTANT
•
No setting contents are determined unless the [Set] button is clicked.
•
To check the image after configuring VIQS, display an H.264 image on the “Live” page, or press the [Confirm] button under “Stream”.
•
The outputted bit rate changes depending on the subject. Confirm the bit rates with actual subjects used when operating the camera.