13.7.1 Configure the settings relating to Panasonic alarm protocol
Panasonic alarm protocol notification
[Panasonic alarm protocol]
Select “On” or “Off” to determine whether or not to provide notification by Panasonic alarm protocol according to the settings for the “Alarm” and “Diag.” checkboxes of “Destination of notification” below.
–
When an alarm is detected (“Alarm”)
–
When a notification of the remaining capacity of the SD memory card has been provided (“Diag.”)
–
When the SD memory card has become full (“Diag.”)
–
When the SD memory card cannot be recognized (“Diag.”)
•
Default: Off
Note
•
When “On” is selected, notification of the alarm occurrence will be provided to the registered destination server addresses in order (to IP address 1 first, to IP address 8 last).
[Additional alarm data]
Determine whether or not to send notifications for VMD alarm detection area numbers with the Panasonic alarm protocol by selecting On/Off.
•
Default: Off
[Destination port]
Select a destination port for the Panasonic alarm protocol from the following.
•
Available range: 1 - 65535
•
Default: 1818
The following port numbers are unavailable since they are already in use.
20, 21, 23, 25, 42, 53, 67, 68, 69, 80, 110, 123, 161, 162, 443, 995, 10669, 10670
[Retry times]
Select a retry time for the Panasonic alarm protocol.
•
Available range: 0-30
•
Default: 2
Destination of notification
[Address 1] - [Address 8]
Enter the destination IP address or host name of the Panasonic alarm protocol from the following. Up to 8 destination server addresses can be registered.
•
[Alarm] checkbox: When the checkbox is checked, the Panasonic alarm notification will be provided upon an alarm occurrence.
•
[Diag.] checkbox: When the checkbox is checked, notification using Panasonic alarm protocol will be provided in the following cases.
–
When notification of the remaining capacity of the SD memory card has been provided
–
When the SD memory card has become full
–
When the SD memory card cannot be recognized
•
[Destination server address]: Enter the destination server address or host name.
–
Available characters: Alphanumeric characters, the colon (:), the period (.), the underscore (_), and the hyphen (-).
To delete the registered destination server address, click the [Delete] button respective to the desired destination server address.
[Notification per VMD area]
Select “On” or “Off” to determine whether or not to set “Notification per VMD area”.
If “Notification per VMD area” is turned “On”, an alarm is notified only when “Alarm area No.” matches “Alarm area” configured by “VMD alarm”. Alarm notifications other than “VMD alarm” are not implemented. When using “Notification per VMD area”, select “On” for “Status” of the alarm area in VMD.
•
Default: Off
[Alarm area No.]
•
Available range: 1-4
•
Default: 1
IMPORTANT
•
When entering the host name of the “Destination server address”, the DNS settings on the [Network] tab of the “Network” page must be configured. (→16.1 Configure the network settings [Network])
•
Confirm that the destination IP addresses are registered correctly. When a registered destination does not exist, notification may be delayed.