11.8 Configure the VIQS setting
Click the [Setup>>] button of “VIQS” on the [Image quality] tab of the “Image/Audio” page. (→11.4 Configure the settings relating to image adjust, zoom/focus, privacy zone, VIQS, and lens distortion compensation [Image quality])
VIQS is an abbreviation of Variable Image Quality on Specified area and is a feature that enables you to change the images of a specified area.
It is possible to enhance the image quality of the specified range within a shooting area (image).
It is also possible to moderate the image data size by lowering the image quality of other areas.
The VIQS setting is available only for H.264 images.
Up to 8 VIQS areas can be set.
To check the image after configuring VIQS, when H.264 images are selected under “Stream”, you can check the image by pressing the [Confirm] button. You can also check by displaying an H.264 image on the “Live” page.
[Area]
When selecting a VIQS area in the screen, it will be numbered as area 1. (Subsequent areas will be numbered in the order of selection.)
[Status]
Select “On” or “Off” to determine whether or not to use the VIQS area.
•
On: The VIQS area will be set.
•
Off: Does not set the VIQS area.
•
Default: Off
[Delete] button
Deletes the VIQS area. Click the button to delete the VIQS area.
[Level]
Configure the difference level in the image quality between specified areas and non-specified areas. The greater the difference level, the more the image quality of the non-specified area is reduced. This makes it possible to moderate the image data size.
0 Min./ 1/ 2/ 3/ 4/ 5 Normal/ 6/ 7/ 8/ 9 Max.
•
Default: 5 Normal
Stream
[H.264(1)]
Select “On” or “Off” to determine whether or not to activate the VIQS function for the transmitted (H.264(1)) images.
The VIQS (H.264(1)) images can be confirmed with the [Confirm] button.
•
Default: Off
[H.264(2)]
Select “On” or “Off” to determine whether or not to activate the VIQS function for the transmitted (H.264(2)) images.
The VIQS (H.264(2)) images can be confirmed with the [Confirm] button.
•
Default: Off
[H.264(3)]
Select “On” or “Off” to determine whether or not to activate the VIQS function for the transmitted (H.264(3)) images.
The VIQS (H.264(3)) images can be confirmed with the [Confirm] button.
•
Default: Off
[H.264(4)]
Select “On” or “Off” to determine whether or not to activate the VIQS function for the transmitted (H.264(4)) images.
The VIQS (H.264(4)) images can be confirmed with the [Confirm] button.
•
Default: Off
IMPORTANT
•
After the VIQS setting is set to “On”, the VIQS area may move out of alignment when the JPEG/H.264 “Image capture mode” setting is changed. Make sure to check the VIQS setting after changing the “Image capture mode” setting.
Note
•
Refer to 11.9 Configure the VIQS area for setting procedure of the VIQS area.
•
When “Off” is selected for “H.264 transmission” of the applicable stream, the stream selection cannot be changed.