16.2.8 Configure the Diffserv settings
The settings relating to Diffserv can be configured on this page. The Diffserv function can be used to set the priority of image/audio data sent from routers.
The priority set to this function must match the DSCP value configured to the router.
When using the Diffserv function, contact the network administrator.
[DSCP(0-63)]
Enter the order of priority for packets.
•
Available values: 0 - 63
•
Default: 0