16.2.6 Configure the settings relating to DDNS
To access this camera via the Internet, it is necessary to configure the settings for the DDNS function.
Refer to 16.5 How to configure the settings relating to DDNS for how to configure the settings relating to DDNS.
[Area]
Select the region where the camera is installed. If the camera is used outside of Japan, select “Global”. If the camera is used in Japan, select “Japan”.
Japan/Global
[Service]
Select the DDNS service to determine whether or not to use DDNS.
•
Off: Does not use the DDNS function.
•
Viewnetcam.com: Uses the “Viewnetcam.com” service.
•
Dynamic DNS Update: Uses Dynamic DNS Update (RFC2136 compliant) without the DHCP cooperation.
•
Dynamic DNS Update(DHCP): Uses Dynamic DNS Update (RFC2136 compliant) with the DHCP cooperation.
•
Default: Off
Note
•
When using Dynamic DNS Update (RFC2136 compliant), refer to the network administrator for whether or not to cooperate with the DHCP.