16.2.7 Configure the settings relating to SNMP
The settings relating to SNMP can be configured on this page. It is possible to check the status of the camera by connecting to the SNMP manager. When using the SNMP function, contact the network administrator.
[Community]
Enter the community name to be monitored.
•
Available number of characters: 0 - 32 characters
•
Default: None (blank)
IMPORTANT
•
When using the SNMP function, it is necessary to enter the community name. When no community name is entered, the SNMP function will not work.
[System name]
Enter a system name to be used to manage the camera with the SNMP function.
•
Available number of characters: 0 - 32 characters
•
Default: None (blank)
[Location]
Enter the name of the location where the camera is installed.
•
Available number of characters: 0 - 32 characters
•
Default: None (blank)
[Contact]
Enter the E-mail address or the phone number of the SNMP manager.
•
Available number of characters: 0 - 255 characters
•
Default: None (blank)