11.5 Adjust the angular field of view using the extra zoom function
Click the [Setup>>] button of “Extra zoom” on the [Image quality] tab of the “Image” page. (→11.4 Configure the settings relating to image adjust, zoom, privacy zone, VIQS, and lens distortion compensation [Image quality])
It is possible to adjust the angular field of view using the extra zoom function.
•
: Click this button to adjust the zoom ratio to the “Wide” side.
•
: Click this button to set the zoom ratio to x1.0.
•
: Click this button to adjust the zoom ratio to the “Tele” side.
•
: Click these buttons to adjust the horizontal/vertical position of the image after zooming.
Note
•
When “2 mega pixel [16:9]” is selected for “Image capture mode”, the maximum zoom ratio of the extra zoom becomes x3.0.
•
When “2 mega pixel [4:3]” or “3 mega pixel [4:3]” is selected for “Image capture mode”, the maximum zoom ratio of the extra zoom becomes x2.5.
•
The maximum zoom ratio of the extra zoom becomes x2.0.
IMPORTANT
•
The positions will move out of alignment if extra zoom settings are configured when the mask area (→11.4.2 Set mask areas), privacy zone (→11.6 Configure the settings relating to the privacy zone (“Privacy zone” setup menu)), VMD area (→13.3 Configure the VMD settings [VMD area]), VIQS area (→11.8 Configure the VIQS area), or cropping area (→14.1 Configure the settings relating to cropping [Cropping]) is configured. To prevent this, perform the setting for the extra zoom function before other settings.
•
When using the lens distortion compensation function, if the extra zoom function is used, the lens distortion compensation function is disabled.