5.2 Transmit images at a designated interval or period (FTP periodic image transmission)
Images can be transmitted at a designated interval or period. To transmit images at a designated interval or period, it is necessary to configure the settings in advance.
FTP server settings and settings relating to FTP periodic transmission image transmission can be configured in the “FTP” section of the [Advanced] tab of the “Network” page. (→16.2.2 Configure the settings related to FTP transmission)
Configure the schedule settings of the FTP periodic image transmission on the “Schedule” page.(→17.1 How to set the schedules)
Note
•
Depending on the line speed or the traffic, images may not be transmitted at the designated interval.
•
When “On” is selected for both the alarm image transmission function and the FTP periodic image transmission function, the alarm image transmission function will be given priority over the FTP periodic image transmission function. Therefore, images may not be transmitted at the interval designated on the “FTP periodic image transmission” setting.