1.3 Monitor cropping images
Full angle images and cropping images can be transmitted at the same time.
The cropping function must be configured in order to transmit cropping images. (→14.1 Configure the settings relating to cropping [Cropping])
Either one of H.264(1), H.264(2), H.264(3), H.264(4), JPEG(1), JPEG(2), or JPEG(3) images or all of H.264(1), H.264(2), H.264(3), and H.264(4) images can be set as cropping images.
By matching the settings of the [Compression] and [Stream]/[Image capture size] buttons on the “Live” page to the stream selected in “Cropping” on the [Cropping] tab, cropping images will be displayed on the [Cropping] display of the “Live” page and the main area.
Cropping
You can crop areas that you want to monitor.
By setting multiple cropping areas, up to 4 areas can be displayed in a sequence.
Sequence display using the cropping function
By selecting the cropping areas for alarm actions, the area you want to monitor (home area) when alarm occurs can be displayed.
Sequence display using the alarm action cropping function
A.
Alarm occurrence
B.
Time while the cropping area is displayed
Note
•
Alarm action cropping can only be used when a setting other than “H.264(all)” is selected for “Cropping”. (→14.1 Configure the settings relating to cropping [Cropping])