4.2 Action at an alarm occurrence
Display the alarm occurrence indication button on the “Live” page
The alarm occurrence indication button will be displayed on the “Live” page at an alarm occurrence. (→1.2 About the “Live” page)
IMPORTANT
•
When “Polling(30s)” is selected for “Alarm status update mode” (→10.1 Configure the basic settings [Basic]), the Alarm occurrence indication button will be refreshed in 30-second intervals. For this reason, it may take a maximum of 30 seconds until the alarm occurrence indication button is displayed on the “Live” page at an alarm occurrence.
Save images on the SD memory card
When an alarm occurs, images (JPEG/H.264) will be saved on the SD memory card. The settings to save images on the SD memory card can be configured on the [SD memory card] tab (→10.3 Configure the settings relating to the SD memory card [SD memory card]) of the “Basic” page and the [Alarm] tab of the “Alarm” page. (→13.2 Configure the settings relating to the camera action on alarm occurrence [Alarm])
Transmit an image onto a server automatically
An alarm image can be transmitted at an alarm occurrence to the server designated in advance. The settings required to transmit an alarm image to a server can be configured in the “Alarm image” section on the [Alarm] tab of the “Alarm” page (→13.2 Configure the settings relating to the camera action on alarm occurrence [Alarm]) and the [Advanced] tab of the “Network” page (→16.2.2 Configure the settings related to FTP transmission).
Notify of alarm occurrences by E-mail
Alarm E-mail (alarm occurrence notification) can be sent at an alarm occurrence to the E-mail addresses registered in advance. Up to 4 addresses can be registered as recipients of the alarm E-mail. An alarm image (still picture) can be sent with the alarm E-mail as an attached file. The settings for alarm E-mail can be configured in the “E-mail notification” section on the [Alarm] tab of the “Alarm” page (→13.2 Configure the settings relating to the camera action on alarm occurrence [Alarm]) and the [Advanced] tab of the “Network” page (→16.2.1 Configure the settings related to sending E-mails).
Notify of alarm occurrences to the designated addresses (Panasonic alarm protocol notification)
This function is available only when a Panasonic device, such as the network disk recorder, is connected to the system. When “On” is selected for “Panasonic alarm protocol notification”, the connected Panasonic device will be notified that the camera is in the alarm state. The settings for Panasonic alarm protocol can be configured in the Panasonic alarm protocol section of the [Notification] tab of the “Alarm” page. (→13.4.1 Configure the settings relating to Panasonic alarm protocol)
Notify of alarm occurrences to the designated HTTP server (HTTP alarm notification)
Alarm occurrence notifications can be sent at an alarm occurrence to the HTTP servers registered in advance. Up to 5 HTTP servers can be registered as recipients of alarm notifications. The URL sent to HTTP servers with alarm notifications can be specified. The settings for HTTP alarm notification can be configured on the [Notification] tab of the “Alarm” page. (→13.4.2 Configure the settings relating to HTTP alarm notification)