11.1 Configure the settings relating to the image capture mode [JPEG/H.264]
Click the [JPEG/H.264] tab on the “Image” page. (→9.1 How to display the setup menu, 9.2 How to operate the setup menu)
[Image capture mode]
Select an image capture mode from the following.
2 mega pixel [16:9]
2 mega pixel [4:3]
3 mega pixel [4:3]*
*Used by super resolution techniques.
•
Default: 2 mega pixel [16:9]
1.3 mega pixel [16:9]
1.3 mega pixel [4:3]
•
Default: 1.3 mega pixel [4:3]
IMPORTANT
•
The positions of areas may move out of alignment when the “Image capture mode” setting is changed when the following area settings are configured. Therefore we recommend that you configure each area setting after configuring the “Image capture mode”.
–
mask area (→11.4.2 Set mask areas)
–
privacy zone (→11.6 Configure the settings relating to the privacy zone (“Privacy zone” setup menu))
–
VMD area (→13.3 Configure the VMD settings [VMD area])
–
VIQS area (→11.7 Configure the VIQS setting)
–
Cropping outlines (→14.1 Configure the settings relating to cropping [Cropping])
Note
•
When “On” is selected for “VIQS” and the setting value for the aspect ratio is changed from “4:3” to “16:9”, make sure that the VIQS setting value does not exceed the maximum designated range.