Viewer software
It is necessary to install the viewer software “Network Camera View 4S” (ActiveX®) to display images on a PC. This software can be installed directly from the camera or by selecting the [Install] button next to [Viewer Software] on the menu of the CD-ROM provided, and then following the on-screen instructions.
IMPORTANT
•
The default setting of “Automatic installation” is “On”. Follow the instructions on Information Bar when the message is displayed on the information bar of the browser.
•
When the “Live” page is displayed for the first time, the install wizard of the ActiveX control required to display images from the camera will be displayed. Follow the instructions of the wizard.
•
When the install wizard is displayed again even after completing the installation of the ActiveX, restart the PC.
•
The viewer software used on each PC should be licensed individually. The number of installations of the viewer software from the camera can be checked on the [Upgrade] tab of the “Maintenance” page (→18.2 Upgrade the firmware [Upgrade]). Refer to your dealer for the software licensing.