11.4.2 Set mask areas
When “Off” is selected for “Wide dynamic range (WDR)” and “Back light compensation (BLC)”, it is possible to compensate for backlight by masking brighter areas.
1.
Display the “Image adjust” setup menu. (→11.4 Configure the settings relating to image adjust, zoom, privacy zone, VIQS, and lens distortion compensation [Image quality])
2.
Click the [Start] button of “Mask area”.
→
Borders will appear and the image displayed on the [Image quality] tab will be divided into 48 (6x8).
3.
Click the divided areas to be masked.
→
The clicked areas will be masked and will become white. To cancel masking, click the area again.
4.
Click the [End] button after completing masking areas.
→
The borders on the image displayed on the [Image quality] tab will disappear.
IMPORTANT
•
The mask area may move out of alignment when the JPEG/H.264 “Image capture mode” setting is changed. Make sure to check the mask area after changing the “Image capture mode” setting.
•
The mask area may move out of alignment when “Extra zoom” is configured. Make sure to check the mask area after configuring “Extra zoom”.
Note
•
When the [Reset] button is clicked, masking for all the masked areas will be canceled.