10.7 Configure the directory of the PC that images will be downloaded to [Log]
Click the [Log] tab on the “Basic” page. (→9.1 How to display the setup menu, 9.2 How to operate the setup menu)
The directory of the PC that images recorded on the SD memory card will be downloaded to can be configured in this section.
Alarm
The settings related to the directory of the PC that recorded images of when alarms occur will be downloaded to can be performed.
[Recording stream 1] - [Name of the destination directory for downloaded images]
Enter the name of the destination directory to which images recorded in the recording stream 1 are to be downloaded. For example, enter “C:\alarm” to designate the folder “alarm” under drive C.
•
Available number of characters: 3 - 128 characters
•
Available characters: Alphanumeric characters, the slash (/), the backslash (\), the colon (:) and the underscore (_).
[Recording stream 2] - [Name of the destination directory for downloaded images]
Enter the name of the destination directory to which images recorded in the recording stream 2 are to be downloaded. For example, enter “C:\alarm2” to designate the folder “alarm2” under drive C.
•
Available number of characters: 3 - 128 characters
•
Available characters: Alphanumeric characters, the slash (/), the backslash (\), the colon (:) and the underscore (_).
Manual/Schedule
The settings related to the directory name of the PC that images recorded by manual saving or schedule saving will be downloaded to can be performed.
Designate the destination folder in the same manner as for “Alarm”.
Note
•
Schedule saving is available only when “H.264(1)”, “H.264(2)”, “H.264(3)”, or “H.264(4)” is selected for “Recording format”.
FTP error
The settings related to the directory name of the PC that recorded images of when FTP errors occur will be downloaded to can be performed.
Designate the destination folder in the same manner as for “Alarm”.
IMPORTANT
•
When “Name w/o time&date” is selected for “File name” of “FTP periodic image transmission”on the [Advanced] tab on the “Network” page, FTP error log and associated images will not be saved. To save them, select “Name w/time&date”. (→16.2.2 Configure the settings related to FTP transmission)
Note
•
When “H.264(1)”, “H.264(2)”, “H.264(3)”, or “H.264(4)” is selected for “Recording format”, “FTP error” is unavailable.
[Permission level of viewing logs]
User level settings for viewing and operating “Log” on the “Live” page can be configured.
1. Level 1 only: only Level 1 users can view and operate the “Log”.
2. Level 2 or higher: only Level 1 and Level 2 users can view and operate the “Log”.
3. All users: all users can view and operate the “Log”. However, only Level 1 and Level 2 users can delete logs, and only Level 1 users can view SD memory card folders.
Default: 1. Level 1 only