16.3 How to configure HTTPS settings
The settings relating to the HTTPS protocol that can enhance the network security by encrypting the access to cameras on this page.
The HTTPS settings will be configured in the following procedure.
Generation of the CRT key (SSL encryption key) (→16.3.1 Generation of the CRT key (SSL encryption key))
Generation of the self-signed certificate (→16.3.2 Generation of the self-signed certificate (security certificate))
Generation of CSR (Certificate Signing Request) (→16.3.3 Generation of CSR (Certificate Signing Request))
Installation of the server certificate (→16.3.4 Installation of the server certificate)
Configuration of the connection protocol (→16.3.5 Configuration of the connection protocol)
Note
•
To use the server certificate, you need to apply for the approval and the issue of server certificate by CA.
•
Either of the self-signed certificate or the server certificate is available. If both of them are installed, the server certificate will be used prior to the self-signed certificate.