2.2 Monitor images on a mobile terminal
It is possible to connect to the camera using a mobile terminal via the Internet and monitor images (MJPEG or JPEG) from the camera on the screen of the mobile terminal. It is also possible to refresh images to display the latest image.
The compatible mobile terminals are shown as follows. (As of September, 2015)
–
iPad, iPhone, iPod touch (iOS 4.2.1 or later)
–
Android™ mobile terminals
When an Android terminal is used, an MJPEG format image is displayed by the Firefox® browser, but a JPEG format image is displayed by the standard browser.
For further information about compatible devices, refer to our website (http://security.panasonic.com/pss/security/support/info.html).
IMPORTANT
•
When the authentication window is displayed, enter the user name and password. The default user name and password are as follows.
User name: admin
Password: 12345
To enhance the security, change the password for the user “admin”. (→15.1 Configure the settings relating to the user authentication [User auth.])
Note
•
It is necessary to configure the network settings of the mobile terminal in advance to connect to the Internet and monitor images from the camera. (→Section 16 Configuring the network settings [Network])
1.
Access to “http://IP address/cam”*1 or “http://Host name registered in the DDNS server/cam” using a mobile terminal.
→
Images from the camera will be displayed.
Live images area
Displays images from the camera.
Operation buttons area
Buttons to operate those functions are displayed.
2.
Click the button of the function that you want to operate.
Each function is explained below.
Resolution control
The resolution can be changed by selecting a resolution setting from the buttons.
Images are displayed in the image capture size selected in “JPEG(1)”, “JPEG(2)”, or “JPEG(3)” of [JPEG] on the [JPEG/H.264] tab.
Note
•
You can change the image size displayed on the mobile terminal by accessing the following addresses.
–
Large display: http://IP address/cam/dl
–
Medium display: http://IP address/cam/dm
–
Small display: http://IP address/cam/ds
•
When the resolution is changed by the resolution control, the displayed resolution changes but the image size remains the same.
•
When the HTTP port number is changed from “80”, enter “http://IP address: (colon) + port number/cam”*1 in the address box of the browser. When using the DDNS function, access to “http://Host name registered in the DDNS server: (colon) + port number/cam”*2.
•
When “HTTPS” is selected for “HTTPS” - “Connection” on the [Advanced] tab of the “Network” page, enter as follows.
“https://IP address: (colon) + port number/cam” or “https://Host name registered in the DDNS server: (colon) + port number/cam”
•
When the authentication window is displayed, enter the user name of an administrator or user and password. Depending on the mobile terminal in use, password entry may be required each time the screen is switched.
•
Depending on the mobile terminal in use, larger size images may not be displayed. In this case, selecting “9 Low” for “Image quality setting” of “JPEG” (→11.2 Configure the settings relating to JPEG images [JPEG/H.264]) may sometimes solve this problem.
•
Depending on the mobile terminal in use or its contract plan, it may be impossible to access.
*1
IP address is the global WAN IP address of the router that can be accessed via the Internet. However, when accessing the same LAN as the camera with a wireless compatible mobile terminal, the IP address is the local IP address.
*2
Only when accessing the camera via the Internet.