18.3 Check the status [Status]
Click the [Status] tab of the “Maintenance” page. (→9.1 How to display the setup menu, 9.2 How to operate the setup menu)
The status of this camera can be checked on this page.
Viewnetcam.com
[Server]
The URL of the “Viewnetcam.com” service server will be displayed.
[Status]
The registration status for the “Viewnetcam.com” will be displayed.
[Personal(Camera) URL]
The URL of the camera registered for “Viewnetcam.com” will be displayed.
UPnP
[Port number(HTTP), Port number(HTTPS)]
The port number that is set for UPnP port forwarding will be displayed.
[Status]
The port forwarding status will be displayed.
[Router global address]
The global address of router will be displayed.
Self check
The self check result of the hardware will be displayed.
Note
•
Refer to our website (http://security.panasonic.com/pss/security/support/info.html) for further information about the contents of the displayed statuses (relating to the “Viewnetcam.com” service, the UPnP function, or the self check).
SD memory card
[Model no.]
Displays the model number of the SD memory card. If model number information could not be obtained, “Read error” is displayed. If the SD memory card is not used, “Not use” is displayed. In other cases “Unknown” is displayed.
[Serial no.]
Displays the serial number of the SD memory card. If model number information could not be obtained, “Unknown” is displayed.
[Remaining capacity]
Displays the remaining capacity and total capacity of the SD memory card. This is the same information that is displayed in [Remaining capacity] of the SD memory card information on the [SD memory card] tab of the “Basic” page.
[Total use time]
Displays the length of time that SD memory card has been inserted into and used with the camera. If the length of time that the SD memory card has been used for cannot be obtained, “Unknown” is displayed. “Total use time” is updated once per hour.
[Number of overwrite times]
Displays the number of overwrite times as calculated from the total capacity of the SD memory card, the number of times the camera has written files to the SD memory card, and the file sizes. If the number of overwrite times cannot be calculated, “Unknown” is displayed.
Note
•
Because the overwrite time values are just estimates calculated by the camera, they may differ to the actual number of overwrite times.
•
When using “SD memory card password lock” and the card’s password does not match, the above information is not displayed.
[No] / [Time & date] / [Description] of the log
Displays the log related to the SD memory card.

Category | Indication | Description
--- | --- | ---
SD memory card | <SD> Format | Successfully formatted the SD memory card.
<SD> Format error | Error occurred when formatting the SD memory card.
<SD> Write-protect ON (Locked card) | A write-protected SD memory card is inserted.
<SD> Detection error | The SD memory card could not be correctly recognized.
<SD> Write error | An error occurred when writing to the SD memory card.
<SD> Read error | An error occurred when reading from the SD memory card.
<SD> Delete error | An error occurred when deleting data from the SD memory card.
<SD> File system error | An error occurred in File system of the SD memory card.
<SD> Undefined error | An error other that the ones above has occurred for the SD memory card.

IMPORTANT
•
In order to be able to correctly use this function, format the SD memory card with the camera before using it.
•
When using SD memory cards that have been used on other devices such as PCs, the correct information may not be able to be displayed.
•
Up to 30 SD memory card logs can be saved to the built-in memory of the camera. When the saved system logs have reached the maximum number, the newer logs will overwrite the older system logs.