9.3 About the setup menu window
[Setup] button
Display the “Setup” page.
[Live] button
Display the “Live” page.
[Basic] button
Displays the “Basic” page. The basic settings such as time and date and camera title, and the settings relating to the SD memory card can be configured on the “Basic” page. (→Section 10 Configure the basic settings of the camera [Basic])
[Image] button
Displays the “Image” page. The settings relating to image quality, image capture size, etc. of JPEG/H.264 camera images can be configured on the “Image” page. (→Section 11 Configure the settings relating to images [Image])
[Multi-screen] button
Displays the “Multi-screen” page. The cameras from which images are to be displayed on a multi-screen can be registered on the “Multi-screen” page. (→Section 12 Configure the multi-screen settings [Multi-screen])
[Alarm] button
Displays the “Alarm” page. The settings relating to alarm occurrences such as settings for the alarm action at an alarm occurrence, the alarm occurrence notification, and the VMD area settings can be configured on the “Alarm” page. (→Section 13 Configure the alarm settings [Alarm])
[Advanced view] button
Displays the “Advanced view” page. The settings relating to cropping can be configured on the “Advanced view”. (→Section 14 Configure the settings related to advanced view [Advanced view])
[User mng.] button
Displays the “User mng.” page. The settings relating to the authentication such as users and PCs restrictions for accessing the camera can be configured on the “User mng.” page. (→Section 15 Configure the settings relating to the authentication [User mng.])
[Network] button
Displays the “Network” page. The network settings and the settings relating to DDNS (Dynamic DNS), SNMP (Simple Network Management Protocol), FTP (File Transfer Protocol), the NTP server, and Diffserv can be configured on the “Network” page. (→Section 16 Configuring the network settings [Network])
[Schedule] button
Displays the “Schedule” page. On the “Schedule” page, it is possible to designate time zones to allow to receive alarm input or to allow to activate the VMD detection function. (→Section 17 Configure the settings relating to the schedules [Schedule])
[Maintenance] button
Displays the “Maintenance” page. System log check, firmware upgrade, status check and initialization of the setup menu can be carried out on the “Maintenance” page. (→Section 18 Maintenance of the camera [Maintenance])
Camera title
The title of the camera whose settings are currently being configured will be displayed.
Setup page
Pages of each setup menu will be displayed. There are tabs for some setup menus.