1.1 Monitor images from a single camera
1.
Start up the web browser.
2.
Enter the IP address designated using the Panasonic “IP Setting Software” in the address box of the browser.
•
Example when entering an IPv4 address: http://URL registered using IPv4 address
http://192.168.0.10/
•
Example when entering an IPv6 address: http://[URL registered using IPv6 address]
http://[2001:db8::10]/
<Example of IPv4 access>
<Example of IPv6 access>
IMPORTANT
•
When the HTTP port number is changed from “80”, enter “http://IP address of the camera + : (colon) + port number” in the address box of the browser. (Example: http://192.168.0.11:8080)
•
When the PC is in a local network, configure the proxy server setting of the web browser (under [Internet Options...] under [Tools] of the menu bar) to bypass the proxy server for the local address.
Note
•
Refer to 16.4 Access the camera using the HTTPS protocol for further information about the case in which “HTTPS” is selected for “HTTPS” - “Connection” on the [Advanced] tab of the “Network” page (→16.1 Configure the network settings [Network]).
3.
Press the [Enter] key on the keyboard.
→
The “Live” page will be displayed. Refer to 1.2 About the “Live” page for further information about the “Live” page.
When “On” is selected for “User auth.”, the authentication window will be displayed before displaying live images for the user name and password entries. The default user name and password are as follows.
User name: admin
Password: 12345
IMPORTANT
•
To enhance the security, change the password for the user name “admin”. It is recommended to change this password periodically.
•
When displaying multiple H.264 images on a PC, images may not be displayed depending on the performance of the PC.
Note
•
The maximum number of concurrent access user is 14 including users who is receiving H.264 images and users who are receiving JPEG images. Depending on the set values for “Bandwidth control(bit rate)” and “Max bit rate (per client)”, the maximum concurrent access number may be 14 or less users. When 14 users are concurrently accessing, the access limit message will be displayed for users who subsequently attempt to access. When “Multicast” is selected for “Transmission type” of “H.264”, only the first user who accessed to monitor H.264 images will be included in the maximum number. The second and subsequent users who are monitoring H.264 images will not be included in the maximum number.
•
When “On” is selected for “H.264 transmission” (→H.264(1)/H.264(2)/H.264(3)/H.264(4)), H.264 images will be displayed. When “Off” is selected, a JPEG image will be displayed. It is possible to display a JPEG image even when “On” is selected for “H.264 transmission”. In this case, the refresh interval of JPEG images will be limited to 5 fps.
•
The refresh interval may become longer depending on a network environment, PC performance, photographic subject, access traffic, etc.
<Refresh interval of JPEG images>
When “On” is selected for “H.264 transmission”
max. 5fps
When “Off” is selected for “H.264 transmission”
max. 30fps