13.1 Configure the settings relating to the alarm action [Alarm]
Click the [Alarm] tab on the “Alarm” page. (→9.1 How to display the setup menu, 9.2 How to operate the setup menu)
The settings relating to the alarm can be configured in this section. Refer to 13.2 Configure the settings relating to the camera action on alarm occurrence [Alarm] for further information about the settings relating to the alarm images.
Alarm
[VMD alarm]
When clicking “VMD >>”, the [VMD area] tab of the “Alarm” page will be displayed. (→13.3.1 Set the VMD areas [VMD area])
[Command alarm]
Select “On” or “Off” to determine whether or not to receive the command alarm.
The command alarm is the function that provides notification of a Panasonic protocol alarm from the other cameras. When “On” is selected, alarm actions will be performed between multiple cameras.
•
Default: Off
[Originating port number]
Select a port number to be used to receive the command alarm.
•
Available range: 1-65535
•
Default: 8181
The following port numbers are unavailable since they are already in use.
20, 21, 23, 25, 42, 53, 67, 68, 69, 80, 110, 123, 161, 162, 443, 554, 995, 10669, 10670, 59000-61000
[Alarm deactivation time]
Configure the duration that detections won’t be made after an alarm is detected. For example, by using this function you can prevent E-mail from being sent too often when E-mail notifications are configured to be sent to cellular phones when an alarm is detected.
5s/ 10s/ 30s/ 1min/ 3min/ 5min/ 10min
Default: 5s
Note
•
The duration that alarm detections are not made can be managed for each type of alarm. For example, during the time when detections for command alarms are not made, detections for VMD alarm can be made.