16.2.8 Configure the Diffserv settings
The settings relating to Diffserv can be configured on this page. The Diffserv function can be used to set the priority of image data sent from routers.
The priority set to this function must match the DSCP value configured to the router.
When using the Diffserv function, contact the network administrator.
[DSCP(0-63)]
Enter the order of priority for packets.
•
Available values: 0 - 63
•
Default: 0