================================================================================

                       Network Disk Recorder (WJ-NX300K)
                                 Read Me First

                         (c) Panasonic Corporation 2017
================================================================================

1. Introduction
   This CD-ROM contains the operating instructions for the Network Disk Recorder.



2. Contents

     CD-ROM
       |
       |--- readme.txt (this file)
       |
       |--- Notes on Windows.pdf
       |
       |--- New Functions.pdf
       |
       |--- Instructions (Folder)
       |       |
       |       |--- English (Folder)
       |       |       |
       |       |       |--- Important Information.pdf
       |       |       |--- Operating Instructions_WJ-NXS series.pdf
       |       |       |--- Operating Instructions_WJ-NXF02.pdf
       |       |
       |       |--- French (Folder)
       |               |
       |               |--- Important Information.pdf
       |               |--- Operating Instructions_WJ-NXS series.pdf
       |               |--- Operating Instructions_WJ-NXF02.pdf
       |               |--- Installation Guide.pdf
       |               |--- Quick Reference Guide.pdf
       |
       |--- OSS (About third-party licenses, Folder)
               |
               |-- gpl.txt
               |-- gpl_1.txt
               |-- lgpl.txt
               |-- license.txt


    ### Notes ###
       Adobe Reader is required to read the instruction files (pdf).
       If Adobe Reader is not installed on your PC, install Adobe Reader. 



3. Notice
   (1) About cameras
     This unit is supported with the following camera models.
     [Panasonic Corporation]
        BB-HCM511          Ver.3.51R00 or later
        BB-HCM527          Ver.3.51R03 or later
        BB-HCM531          Ver.3.51R00 or later
        BB-HCM547          Ver.3.51R03 or later
        BB-HCM580          Ver.3.51R00 or later
        BB-HCM581          Ver.3.51R00 or later
        BB-HCM701          Ver.4.30R00 or later
        BB-HCM705          Ver.4.30R00 or later
        BB-HCM715          Ver.4.30R00 or later
        BB-HCM735          Ver.4.30R00 or later
        WJ-GXE100
        WJ-GXE500
        WV-NP240 series
        WV-NP502
        WV-NS202A
        WV-NW502S
        WV-S1111           Ver.1.70 or later
        WV-S1112 series    Ver.1.70 or later
        WV-S1131           Ver.1.70 or later
        WV-S1132 series    Ver.1.70 or later
        WV-S1511 series    Ver.1.70 or later
        WV-S1531 series    Ver.1.70 or later
        WV-S2110 series    Ver.1.70 or later
        WV-S2111L          Ver.1.70 or later
        WV-S2130 series    Ver.1.70 or later
        WV-S2131 series    Ver.1.70 or later
        WV-S2211L          Ver.1.70 or later
        WV-S2231L          Ver.1.70 or later
        WV-S2511LN         Ver.1.70 or later
        WV-S2531 series    Ver.1.70 or later
        WV-S4150
        WV-S4550L series
        WV-S6111           Ver.1.70 or later
        WV-S6130           Ver.1.70 or later
        WV-S6131           Ver.1.70 or later
        WV-S6530N          Ver.1.70 or later
        WV-SC384
        WV-SC385
        WV-SC386
        WV-SC387 series
        WV-SC588 series
        WV-SF132
        WV-SF135
        WV-SF138
        WV-SF332
        WV-SF335
        WV-SF336
        WV-SF342
        WV-SF346
        WV-SF438           Ver.1.50 or later
        WV-SF448           Ver.1.50 or later
        WV-SF538
        WV-SF539
        WV-SF548
        WV-SF549
        WV-SFN110
        WV-SFN130
        WV-SFN310 series
        WV-SFN311 series
        WV-SFN480          Ver.2.53 or later
        WV-SFN531
        WV-SFN611L
        WV-SFN631L
        WV-SFR310 series
        WV-SFR311 series
        WV-SFR531
        WV-SFR611L
        WV-SFR631L
        WV-SFV110 series
        WV-SFV130 series
        WV-SFV310 series
        WV-SFV311 series
        WV-SFV481          Ver.2.53 or later
        WV-SFV531
        WV-SFV611L
        WV-SFV631L series
        WV-SFV781L         Ver.2.53 or later
        WV-SMR10 series
        WV-SP102
        WV-SP105
        WV-SP302
        WV-SP305
        WV-SP306
        WV-SP508
        WV-SP509
        WV-SPN310 series
        WV-SPN311 series
        WV-SPN531 series
        WV-SPN611
        WV-SPN631
        WV-SPV781L         Ver.2.53 or later
        WV-SPW311AL
        WV-SPW312L
        WV-SPW531AL
        WV-SPW532L
        WV-SPW611 series
        WV-SPW631L series
        WV-ST162
        WV-ST165
        WV-SUD638
        WV-SW115
        WV-SW152 series
        WV-SW155 series
        WV-SW158
        WV-SW172
        WV-SW174W
        WV-SW175
        WV-SW314
        WV-SW316 series
        WV-SW352
        WV-SW355
        WV-SW395 series
        WV-SW396 series
        WV-SW397 series
        WV-SW458 series    Ver.1.50 or later
        WV-SW558
        WV-SW559
        WV-SW598 series
        WV-V1170
        WV-V1330L1
        WV-V1330LK
        WV-V2530L1
        WV-V2530LK
        WV-V6430L
        WV-X4170
        WV-X4171
        WV-X4571L series
        WV-X6511N          Ver.1.70 or later
        WV-X6531N          Ver.1.70 or later

        * The following cameras are not listed in the "Model" of "Registered
          information". To use these cameras, detect them and register on "Easy
          Start" or "Detect cameras" of "Camera registration".
           - BB-HCM701
           - BB-HCM705
           - BB-HCM715
           - BB-HCM735
           - WV-NP240 series
           - WV-NS202A

        * The following cameras, when the compression method is H.264 and the frame
          rate is set to 3ips or low, will transmit the images at 5ips.
           - BB-HCM701
           - BB-HCM705
           - BB-HCM715
           - BB-HCM735

        * The following cameras support MJPEG compression method only.
           - BB-HCM511
           - BB-HCM527
           - BB-HCM531
           - BB-HCM547
           - BB-HCM580
           - BB-HCM581

        * WV-SW174W supports wired network only.

        * Depending on the setting of "CH selection" for WJ-GXE500, the images
          may not be transmitted at the specified frame rate. Refer to the
          operating instructions of WJ-GXE500 for details.

        * To register more than one camera connected to the same WJ-GXE500, set
          the same value to each camera on following settings.
           - Compression
           - Image capture size
           - Frame rate
           - Image quality

        * To register WV-SF438, WV-SF448 and WV-SW458 series, specify the image
          capture mode together.
           - (DP)     :<Ceiling> Double Panorama
           - (P)      :<Wall> Panorama
           - (FE)     :<Ceiling> Fisheye
           - (4PTZ)   :<Ceiling> Quad PTZ
           - (1PTZ)   :<Ceiling> Single PTZ
           - (FE+4PTZ):<Ceiling> Fisheye + Quad PTZ
           - -1~-4    :<Ceiling> VGA Quad streams
           * Camera operations are available in "Single PTZ" and "Quad PTZ" mode.
           * All four areas are subject to the operations of reset zoom factor to
             x1 in "Quad PTZ" mode.
           * When change the image capture mode or image capture size (resolution),
             the mounting position returns to the default settings described above.
           * The maximum recording rate is 15 ips in "Fisheye + Quad PTZ" mode.

        * To register WV-SFN480, WV-SFV481, WV-S4150, WV-S4550L series, WV-X4170,
          WV-X4171 and WV-X4571L series, specify the image capture mode together.
           - (FE)     :<Ceiling> Fisheye
           - (DP)     :<Ceiling> Double Panorama
           - (P)      :<Wall> Panorama
           - (4PTZ)   :<Ceiling> Quad PTZ
           - (1PTZ)   :<Ceiling> Single PTZ
           - (FE+DP)  :<Ceiling> Fisheye + Double Panorama
           - (FE+P)   :<Wall> Fisheye + Panorama
           - (FE+4PTZ):<Ceiling> Fisheye + Quad PTZ
           - -1~-4    :<Ceiling> Quad streams
           * Camera operations are available in "Single PTZ", "Quad PTZ", 
             "Fisheye + Quad PTZ" and "Quad streams" mode.
           * Click the [x1] button of Zooming to reset the zoom factor to x1 for 
             all 4 areas in "Quad PTZ" and "Fisheye + Quad PTZ" mode.
           * When change the image capture mode or image capture size (resolution),
             the mounting position returns to the default settings described above.

        * To use RS-485 output unit with WV-SPN611 or WV-SPN631, 
          select "WV-SPN611(R48)" or "WV-SPN631(R48)" severally.

        * When the Super Dynamic is set to On for WV-X4170, WV-X4171 and WV-X4571L
          series in the Camera setup, the wide dynamic range is set to On.

     [AXIS Communications]
        AXIS M7001
        AXIS P3384 Ver.5.40.11 (ONVIF)
        AXIS M5013 Ver.5.50.3  (ONVIF)
        AXIS P1346 Ver.5.40.9.5(ONVIF)
        * AXIS M7001 supports MJPEG compression method only.

     [Sony Corporation]
        SNC-CH210 Ver.1.78.00 (ONVIF)
        SNC-ER520 Ver.1.78.00 (ONVIF)
        SNC-EM600 Ver.2.8.0   (ONVIF)

     [VIVOTEK INC.]
        IP8162 Ver.IP8162-VVTK-0200 (ONVIF)

   (2) About image capture size
     The supporting resolution depends on the compression method.
        [H.265]
          H.265(1) stream
            QXGA(2048x1536)
            UXGA(1600x1200)
            SXVGA(1280x960)
            SVGA(800x600)
            VGA(640x480)
            FHD(1920x1080)
            HD(1280x720)
            HVGAW(640x360)
            5M(2192x2192)
            1.6M(1280x1280)
            2M(1080x1920)
            1M(720x1280)
            0.2M(360x640)

          H.265(2) stream
            VGA(640x480)
            HVGAW(640x360)
            0.2M(360x640)

        * This unit uses H.265(1) stream for live viewing on a 1-screen, and uses
          H.265(2) stream for live viewing on a multiscreen.

        [H.264]
          H.264(1) stream
            12M(4000x3000)
            5M(2560x1920)
            QXGA(2048x1536)
            UXGA(1600x1200)
            SXVGA(1280x960)
            SVGA(800x600)
            VGA(640x480)
            4KUHD(3840x2160)
            WQHD(2560x1440)
            FHD(1920x1080)
            HD(1280x720)
            HVGAW(640x360)
            9M(2992x2992)
            8M(2816x2816)
            5M(2192x2192)
            4M(2048x2048)
            1.6M(1280x1280)

          H.264(2) stream
            VGA(640x480)
            HVGAW(640x360)
            0.4M(640x640)

        * This unit uses H.264(1) stream for live viewing on a 1-screen, and uses
          H.264(2) stream for live viewing on a multiscreen.

        [JPEG]
          12M(4000x3000)
          5M(2560x1920)
          QXGA(2048x1536)
          UXGA(1600x1200)
          SXVGA(1280x960)
          SVGA(800x600)
          VGA(640x480)
          9M(2992x2992)
          8M(2816x2816)
          5M(2192x2192)
          4M(2048x2048)
          1.6M(1280x1280)
          0.4M(640x640)

   (3) About Live audio / Audio rec.
     [Panasonic Corporation]
       The Live audio / Audio rec. functions are available when the camera supports
       audio transmission function.
        * For WJ-GXE500, only CH1 supports these functions.
        * For "Quad streams" mode of WV-SFN480 and WV-SFV481, only CH1 supports
          these functions.

   (4) About camera models supported VMD search function
     [Panasonic Corporation]
       The displaying VMD information on a timeline and VMD search function are
       available when the camera supports VMD information addition.
        * The "Quad PTZ", "Single PTZ" and "VGA Quad streams" mode of WV-SF438,
          WV-SF448 and WV-SW458 series don't support this function.

   (5) About camera categories of camera registration
     The correspondence table of camera categories excluding model numbers
     and camera models is following.
        i-PRO(Old)         WV-NP240 series, WV-NS202A
        i-PRO(St1Only)     (i-PRO Network Cameras supporting H.264 stream output)
        i-PRO(Unknown)     (Unknown i-PRO Network Cameras)
        GXE500-1           WJ-GXE500(CH1)
        GXE500-2           WJ-GXE500(CH2)
        GXE500-3           WJ-GXE500(CH3)
        GXE500-4           WJ-GXE500(CH4)
        HCM3**             (No model No.)
        HCM5**             BB-HCM511, BB-HCM527, BB-HCM531, BB-HCM547,
                           BB-HCM580, BB-HCM581
        HCM7**             BB-HCM701, BB-HCM705, BB-HCM715, BB-HCM735
        AXIS               Manufactured by AXIS Communications
        ONVIF              ONVIF standard cameras

        * If the correspondence table of camera categories are selected,
          some functions may not operate correctly depending on the models.
          It is recommended to register cameras by "Easy Start".

        * When "i-PRO(St1Only)" for camera categories and "H.264" for compression
          are selected, this unit uses only H.264(1) stream for live viewing and 
          recording.

   (6) About register camera home position
     On the following camera models, preset position number 0 is registered as 
     home position.
        BB-HCM511
        BB-HCM527
        BB-HCM547
        BB-HCM580
        BB-HCM581
        BB-HCM715
        BB-HCM735

   (7) About "Easy Start" function
     [Panasonic Corporation]
        - Only CH1 of "WJ-GXE500" can be detected by this function.
          (To register camera channel 2 to 4, select "GXE500-2" to "GXE500-4"
          for each camera channel on "Model" - "Registered information" page -
          [Camera registration] tab.)
        - WV-SF438, WV-SF448 and WV-SW458 series can be detected as
          "<Ceiling> Double Panorama".
        - WV-SFN480, WV-SFV481, WV-S4150, WV-S4550L series, WV-X4170, WV-X4171
          and WV-X4571L series can be detected as "<Ceiling> Fisheye".
        - The i-PRO network cameras that is not supported yet can be detected
          as "i-PRO(Unknown)". To register them, select the alternative model
          for each camera on "Model" - "Registered information" page - 
           [Camera registration] tab.

     [AXIS Communications]
        - Only ONVIF standard cameras can be detected by this function.

     [Sony Corporation]
        - Only ONVIF standard cameras can be detected by this function.

     [VIVOTEK INC.]
        - Only ONVIF standard cameras can be detected by this function.

   (8) About the optional software
     [Panasonic Corporation]
        WV-ASM300         Ver.1.30 or later

   (9) About recommended cameras supporting the face detection function
     The face matching function is supported with the following camera models.
     [Panasonic Corporation]
        WV-SP305          Ver.2.13 or later
        WV-SP306          Ver.2.13 or later
        WV-SFV631LT       Ver.1.87 or later
        WV-SPN310 series  Ver.1.87 or later
        WV-SPN311 series  Ver.1.87 or later
        WV-SPN531 series  Ver.1.87 or later
        WV-SPN611         Ver.1.87 or later
        WV-SPN631         Ver.1.87 or later
        WV-S1111          Ver.1.70 or later
        WV-S1112          Ver.1.70 or later
        WV-S1131          Ver.1.70 or later
        WV-S1132          Ver.1.70 or later
        WV-S2531LTN       Ver.1.70 or later
        * A megapixel compatible Vari-Focal lens with 8-fold or more magnification
          is recommended. 
        * WV-SFV631LT and WV-S2531LTN can be used indoor for this purpose.
        
        WV-SC385          Ver.2.13 or later
        WV-S6130          Ver.1.70 or later
        * Use as fixed camera.

4. Using ONVIF standard cameras
     This unit is equipped ONVIF Client function of ONVIF Profile S and can connect
     to cameras supporting ONVIF Profile S. The available camera models are mentioned
     above in "3. Notice"-"(1) About cameras".

     This unit supports following functions to the ONVIF standard cameras.
      (1) Auto camera detection
      (2) Register the camera manually
      (3) Display live camera image, recording and playback camera image
          - Video compression format:H.264,  MJPEG
            * not support H.265
          - Image capture size:
              H.264  SXVGA(1280x960), VGA(640x480)
                     FHD(1920x1080), HD(1280x720), HVGAW(640x360)
              MJPEG  SXVGA(1280x960), VGA(640x480)
          - Frame rate:
              H.264  30ips, 15ips, 10ips, 5ips, 3ips, 1ips
              MJPEG  5ips, 3ips, 1ips
          - Image quality:
              H.264  XF(Extra Fine), SF(Super Fine), FQ(Fine), NQ(Normal)
              MJPEG  SF(Super Fine), FQ(Fine), NQ(Normal)
      (4) Output live audio, recording and playback audio
          - Audio compression format: G.711
      (5) Camera control (Pan, Tilt, Zoom, Register and call preset position) 
      (6) Receive the events
      (7) User authentication
          - Authentication method: Basic Authentication, Digest Authentication,
                                   no authentication

     To use ONVIF standard cameras, this unit has following notice. 

     [Common]
       - Depending on which version or function of ONVIF the camera supports,
         this unit may not connect to the cameras or not work correctly. And
         some functions may work slowly.

       - Set the IP address to the cameras in advance. For further information,
         refer to the operating instructions of the cameras in use.

       - This unit receives events which are sent by ONVIF standard camera and
         treats them as "Camera site alarm (ONVIF)". Set the camera in use
         whether or not to provide an alarm notification when an event occurs.

       - A preset position number 0 is registered as home position.

       - Set the same time zone with this unit to the cameras.

       - Adjust the time and date of the camera to the clock of this unit.

       - When the compression method of the camera is "MJPEG", the image capture
         size is "SXVGA(1280x960)" and the image quality is "SF", set 3ips or low
         for the frame rate.

       - When a part of the camera image broken is displayed or whole image isn't 
         displayed, set the image quality to low.

     [AXIS Communications]
       - Set the following items to the camera in use.
           *1 Choose Setup > System Options > Network > TCP/IP > Basic, check
              "Use the following IP address" and specify the IP address for "IPv4
              Address Configuration".
           *2 Choose Setup > System Options > Security > ONVIF, add ONVIF user
              (User group: Administrator).

       - AXIS P3384 Ver.5.40.11 and AXIS M5013 Ver.5.50.3 are impossible to connect
         with ONVIF by default. It is necessary to configure the settings(*1,*2).

     [Sony Corporation]
       - Register the user name and password of camera into this unit.

       - When an event occurs in the camera, this unit may not receive the event
         or receive the event which is not presumed.

       - The camera may be disconnected from this unit when restart this unit or 
         change the system deployment such as changing camera configuration or 
         plugging and unplugging the network cable. In this case, the connection
         may recover after turning off and on the camera or resetting to factory
         default settings.

    * ONVIF and the ONVIF logo are trademarks of ONVIF Inc.


5. About third-party software licenses

      The software contains third-party software programs licensed under GPL/LGPL, etc.
      The licenses can be found at OSS folder in this CD-ROM.
      And also you can get GPL/LGPL source files and the copyright notice list
      from the following site at least three years from delivery of products.
      http://security.panasonic.com/pss/security/support/inquiry.html


6. Copyright
   Except for the software stipulated in Article 5, all copyrights and
   intellectual rights for this software incorporated herein are
   the property of, or under license to Panasonic Corporation or the third parties.
   Those rights are never transferred to the customers.

   Anything in the foregoing to the contrary notwithstanding, Panasonic
   Corporation shall have no obligation for any defects in the physical
   media on which the Program is furnished resulting from your storage thereof,
   or for defects that have been caused by operation of the physical media
   otherwise than as, or in environmental conditions other than those,
   specified by Panasonic Corporation by accident, misuse,
   neglect, abuse, mishandling, misapplication, modification, alteration acts
   of God or by improper installation or maintenance.

   PANASONIC CORPORATION ASSUMES NO RISK OF, AND SHALL
   NOT IN ANY CASE BE LIABLE FOR, ANY DAMAGE, INCLUDING, WITHOUT
   LIMITATION ANY SPECIAL, INCIDENTAL, CONSEQUENTIAL OR PUNITIVE DAMAGES,
   ARISING FROM BREACH OR WARRANTY OR CONTRACT, NEGLIGENCE OR
   ANY OTHER LEGAL THEORY, INCLUDING WITHOUT LIMITATION, LOSS OF
   GOODWILL, PROFITS OR REVENUE, LOSS OF THE PROGRAM, PRODUCT OR
   ANY ASSOCIATED EQUIPMENT, COST OF CAPITAL, COST OF ANY
   SUBSTITUTE EQUIPMENT, FACILITIES OR SERVICES, DOWNTIME COSTS,
   OR CLAIMS OF ANY PARTY DEALING WITH YOU FOR SUCH DAMAGES.


Ver.1.03
