i-PRO WV-XAE207W AI OCCUPANCY DETECTION APPLICATION SOFTWARE
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 13 VIDEO SURVEILLANCE CONTROL AND MANAGEMENT SYSTEMS

This specification is intended for use by the design/construction professional and any user of i-PRO Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormatTM 2014 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	 i-PRO Sensing Solutions Co., Ltd

B.	Provide Video Surveillance Products from single source manufacturer 

2.2	i-PRO WV-XAE207W AI OCCUPANCY DETECTION APPLICATION SOFTWARE
A.	GENERAL CHARACTERISTICS

1.	The AI Occupancy Detection application software shall perform high precision with deep learning technology.

2.	The AI Occupancy Detection application software shall detect if the set number of people is exceeded continuously in the target area during the set time period. 

3.	The AI Occupancy Detection application software shall set a maximum of 4 detection areas. 

4.	The AI Occupancy Detection application software shall allow the areas to be set to overlap each other.

5.	The AI Occupancy Detection application software shall support up to 16 polygonal areas (up to 16 vertices each) being specified in an image in the detection area settings.

6.	The AI Occupancy Detection application software shall set alarm conditions (number of people and time) for each area.

7.	The AI Occupancy Detection application software shall enable or disable settings for specific areas, and the status can be confirmed on the screen. Areas where the settings are enabled are indicated by solid lines and those where they are disabled are indicated by dotted lines.

8.	The AI Occupancy Detection application software shall trigger the alarm by a set number of people (between 1 and 40).

9.	The AI Occupancy Detection application software shall have a detectable angle of view of 45° or less.

10.	The AI Occupancy Detection application software shall detect the following body size:	Shoulder width: 32-1400 pixels (FHD model); 43-1866 pixels (5M model); 64-2800 pixels (4K model)

11.	The AI Occupancy Detection application software shall activate the alarm after a specific period of time elapses when the number of people set for detection in an area is reached. A period of 1 to 600 (seconds) can be set.

12.	The AI Occupancy Detection application software shall send congestion information on up to four areas separately by HTTP.

13.	The AI Occupancy Detection application software shall use SSL to send congestion information.

14.	The AI Occupancy Detection application software shall support selecting the transmission interval from the following six settings:
　　　　Transmission interval: 1 min, 5 min, 10 min, 15 min, 30 min, 60 min

15.	The AI Occupancy Detection application software shall require that the installation location be indoors (including the under-eave areas not exposed to direct sunlight).

16.	The AI Occupancy Detection application software shall require illuminance of 50 lux or above (around the subject).

B.	SYSTEM REQUIREMENT
1.	Supported network cameras
WV-X2571LN / WV-X2551LN / WV-X2271L /WV-X2251L / WV-X1571LN / WV-X1551LN 
WV-S2536LTN / WV-S2536LN / WV-S2536L / WV-S2236L / WV-S2136L / WV-S2136 / 
WV-S1536LTN / WV-S1536L

C.	PRODUCTS LINE-UP
1.	None