i-PRO WV-ASM300 MANAGEMENT AND MONITORING SOFTWARE
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 19 DIGITAL VIDEO RECORDERS AND ANALOG RECORDING DEVICES

This specification is intended for use by the design/construction professional and any user of i-PRO Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormatTM 2014 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	i-PRO Sensing Solutions Co., Ltd. 

B.	Provide Video Surveillance Camera from single source manufacturer 

2.2	i-PRO WV-ASM300 MANAGEMENT AND MONITORING SOFTWARE

A.	GENERAL CHARACTERISTICS
1.	The Management and Monitoring software shall support up to 500 recorders with an optional extension license.

2.	The Management and Monitoring software shall support up to 32,000 cameras via recorder with an optional extension licenses.

3.	The Management and Monitoring software shall manage a network disk recorder and DVR (for analog cameras) concurrently. 

4.	The Management and Monitoring software shall be operated with a controller.

5.	The Management and Monitoring software shall offer an operation screen, a live screen and a map screen. 

6.	The Management and Monitoring software shall automatically switch video streams depending on the number of the number of split-screen to save the bandwidth.

7.	The Management and Monitoring software shall be equipped with a thumbnail search function to find a search point easily. 

8.	The Management and Monitoring software shall be equipped with cropping function for 4K image and the dewarping function for 360-degree image. 

9.	The Management and Monitoring software shall offer the download and playback function of mp4 videos. 

10.	The Management and Monitoring software shall be equipped with an analytics function (people counting and heat-mapping). 

11.	The Management and Monitoring software shall be equipped a local authentication and an authentication with Active Directory.

12.	The Management and Monitoring software shall support the user level management.

13.	The Management and Monitoring software shall receive encrypted stream and play it. 

14.	The Management and Monitoring software shall realize SSL / TLS communication with CA certificate.

15.	The Management and Monitoring software shall offer an optional image visibility enhancement function for monitoring images more clearly in bad weather.

16.	The Management and Monitoring software shall offer an optional face search function for monitoring using a person’s face. 

B.	MANAGEMENT AND MONITORING SOFTWARE
1.	Inputs			
a.	Camera		Up to 1,280 cameras with direct communication
b.	Recorder		Up to 500 recorders
c.	Encoder		Up to 320 encoders
d.	Decoder		Up to 10 decoders
2.	Operation device		Up to 1 controller

C.	FUNCTIONS
1.	Display
a.	Multi monitor		Operation window, Up to 4 Live windows, Map window
b.	Multiscreen Display   Up to 64 multiscreen 
c.	Camera control	Panning, Tilting, Zoom, Focus, Brightness, Preset position call
and program (up to 256), Auto mode, Click centering, Wheel
zoom, Zoom reset, Auto Back Focus
d.	Recorder control	Play, Reverse Play, Pause, Stop, Fast Forward, Fast Reverse, 
Previous Record, Next Record, Previous Image, Next Image, Go to Date, Go to Last (Jumps to 30 seconds before the record end)

2.	Live and playback
a.	Image format		H.265, H.264, MJPEG, MPEG4
b.	Frame rate		Up to 60ips (Depending on the Camera)
c.	Audio		G.726 (ADPCM), 32kbps, AAC-LC
d.	Search mode	Date and time (Calendar), Timeline, Video Motion Detection
(VMD) log list
e.	De-warp		1 de-warped live and playback of fisheye images

3.	Management
a.	User registration	Up to 32 users
b.	Authentication	ID and Password
c.	User level		Administrator and customizable 6-level user authentication
d.	Quick setup		Set-up wizard with Automatic camera / recorder detection

D.	SOFTWARE OPTIONS
1.	WV-ASM202 Extension software for expanding the maximum numbers of screens
2.	WV-ASM203 Extension software for expanding the maximum numbers of devices
3.	WV-ASM204 Extension software for Decoder registration
4.	WV-ASM205 Extension software for adding Visibility enhancement function
5.	WV-ASM231 Extension software for using Face Recognition System
6.	WV-ASM306 Extension software for controlling Video Insight server