**i-PRO WV-S1136A INDOOR BOX NETWORK CAMERA WITH AI ENGINE**

**TECHNICAL SPECIFICATIONS**

**DIVISION 28 – ELECTRONIC SAFETY AND SECURITY**

**28 20 00 ELECTRONIC SURVEILLANCE**

**28 23 00 VIDEO SURVEILLANCE**

**28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS**

*This specification is intended for use by the design/construction professional and any user of i-PRO Security products to assist in developing project specifications for security and video surveillance systems.*

*Specifier Notes: This guide specification incorporates CSI MasterFormatTM 2014 Edition Numbers and Titles.*

*Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.*

**PART 1 GENERAL**

* 1. **SUMMARY**
  2. **WARRANTY**

1. Provide manufacturer's standard warranty.

**PART 2 PRODUCTS**

1. **MANUFACTURERS**
   1. i-PRO Co., Ltd.
   2. Provide Video Surveillance Camera from single source manufacturer

**i-PRO WV-S1136A INDOOR BOX NETWORK CAMERA WITH AI ENGINE**

1. **GENERAL CHARACTERISTICS**
2. The Indoor Box Camera shall deliver H.265 stream and H.264 stream.
3. The Indoor Box Camera shall produce a resolution of 1920 x 1080 pixels at up to 60fps

with a 16:9 aspect ratio.

1. The Indoor Box Camera shall utilize an approximate 1/2.8 type high sensitivity CMOS image sensor. The Indoor Box Camera shall built-in AI engine to enable analytical applications on network edge. Built-in AI engine supports the detecting suspicious changes in captured scenes, optimizing the image settings of the camera (based on captured scene analysis) for better image usability, and optimizing video compression through captured scenes to save bandwidth.
2. The Indoor Box Camera shall be enabled to install the optional analytics applications with including developed by third party companies using this camera's SDK.
3. The Indoor Box Camera shall feature a 144dB wide dynamic range based on Enhanced Super Dynamic and built-in AI engine and Adaptive Black Stretch technology (ABS).
4. The Indoor Box Camera shall produce a color image with a minimum illumination of 0.006 lux and a monochrome image with 0.004 lux at F1.2, shutter speed of 1/30s and AGC 11.
5. The Indoor Box Camera shall offer a built-in IR illumination to produce a clear monochrome image in zero lux conditions with 40m (131feet) irradiation distance.
6. The Indoor Box Camera shall be equipped with a special coated cover for increasing the operational utility of outdoor cameras in rainy weather.
7. The Indoor Box Camera shall generate multiple simultaneous video streams of up to four (4) H.265 (Main profile) or H.264 (High profile) streams and JPEG streams.
8. The Indoor Box Camera shall be equipped with AI intelligent auto mode which is the technology for shooting license plate and person’s face more clearly.
9. The Indoor Box Camera shall be equipped with GOP controls including smart facial coding and frame control and it reduce bit rate by controlling the image quality of still areas, moving areas, and faces with AI ​​engine.
10. The Indoor Box Camera shall be equipped with corridor mode enables the capture of a more

vertically oriented area than the normal format would allow.

1. The Indoor Box Camera shall produce encrypted stream.
2. The Indoor Box Camera shall realize SSL / TLS communication with CA certificate.
3. The Indoor Box Camera shall be rated to IK10 vandal resistance.
4. The Indoor Box Camera shall be rated to IP66 and NEMA 4X standard against water and dust ingress.
5. A user shall be able to view videos on a PC using a browser.
6. A user shall be able to view videos on a smartphone and tablet using viewer software for iPhone and Android.
7. The Indoor Box Camera shall offer Video Motion Detection (VMD) with four (4) programmable detection areas, 15 steps sensitivity level and 10 steps detection size.
8. The Indoor Box Camera shall offer Scene Change Detection (SCD) is possible to issue an alarm when a camera is covered with something, or the camera direction is changed to shoot a different subject.
9. The Indoor Box Camera shall have Fog compensation function.
10. The Indoor Box Camera shall have High light compensation (HLC) function.
11. The Indoor Box Camera shall have Super Chroma Compensation (SCC) which realizes a better color reproducibility in the low illumination.
12. The Indoor Box Camera shall provide up to eight (8) areas of electronic privacy masking.
13. The Indoor Box Camera shall offer the prioritized stream control which transmits a video stream to a specified client PC or recorder preferentially.
14. The Indoor Box Camera shall have an SD memory card slot that supports SD, SDHC and SDXC memory cards for local storage.
15. The Indoor Box Camera shall offer full-duplex bi-directional audio communication capability between the camera and monitoring site.
16. The Indoor Box Camera shall have three (3) alarm sources of terminal input, VMD, and command alarm that activate the processes such as SDXC/ SDHC/SD memory recording, E-mail notification, HTTP alarm notification, Indication on browser, FTP image transfer and TCP alarm notification output.
17. The Indoor Box Camera shall conform to the ONVIF G / M / S / T standard.

|  |  |
| --- | --- |
| **CAMERA** | |
| Minimum Image Sensor | Approx. 1/2.8 type CMOS image sensor |
| Minimum Illumination   * + - 1. Color       2. BW | Color: 0.006 lx (30IRE, F1.2, 1/30s)  Color: 0.008 lx (50IRE, F1.2, 1/30s)  BW: 0.004 lx (50IRE, F1.2, 1/30s) |
| Color/BW (ICR) | Off / On / Auto1 (Normal) / Auto2 (IR Light) / Auto3 (SCC) |
| White Balance | ATW1/ ATW2/ AWC |
| Dynamic Range | Max.144 dB (Super Dynamic: On, Level 31) |
| Image Rotation | 0 ° / 90 ° / 180 ° / 270 ° |
| AI Analytics | AI Video Motion Detection, AI Privacy Guard, AI Face Detection, AI People Detection, AI Vehicle Detection, AI Non mask Detection, AI Occupancy Detection, AI Scene Change Detection  For details [AI Surveillance](https://i-pro.com/global/en/surveillance/products/i-pro-ai-application) 3rd party applications are also available. [AI Surveillance List](https://i-pro.com/global/en/surveillance/i-pro-application-platform/application-list) |
| AI Sound Classification | Gunshot, Yell, Vehicle horn, Glass break |

|  |  |
| --- | --- |
| **LENS** | |
| Focus Adjustment | Auto back focus / Manual / Adjusting method (Auto / Preset / Fix) |

|  |  |
| --- | --- |
| VIDEO | |
| Image Resolution   1. 16:9 aspect ratio 2. 4:3 aspect ratio | [16:9 mode (60 fps mode)] \*2, [16:9 mode (30 fps mode)], [16:9 mode (50 fps mode)] \*2, [16:9 mode (25 fps mode)], 1920x1080, 1280x720, 640x360, 320x180  [4:3 mode (30 fps mode)], [4:3 mode (25 fps mode)], 1280x960, VGA, QVGA, [4:3 mode (15 fps mode)], [4:3 mode (12.5 fps mode)], 2048x1536\*5, 1280x960, VGA, QVGA |
| H.265/ H.264   1. Transmission Mode 2. b. Transmission Type | Constant bit rate / VBR / Frame rate / Best effort  Unicast port (AUTO) / Unicast port (MANUAL) / Multicast |
| JPEG Image Quality | 10 steps |
| Smart Coding   1. GOP (Group of Picture) control 2. Smart VIQS 3. Smart P-picture control | Off/ Low (Variable GOP 1s-8s)/ Mid (Variable GOP 4s-16s)/ Advanced (Indoor Box GOP 60s w/1s key-frame)/ Frame rate control (Variable GOP 4s-16s with frame rate control) \*Advanced and Frame rate control are only available with H.265.  On (High)/On (Low)/Off, Up to 8 zones available  On/Off |

|  |  |
| --- | --- |
| AUDIO | |
| Audio Compression | G.726 (ADPCM): 16 kbps / 32 kbps  G.711: 64 kbps AAC-LC: 64 kbps / 96 kbps / 128 kbps |
| Audio Detection | On / Off |
| Audio Transmission Mode | Off / Mic (Line) input / Audio output / Interactive (Half duplex) / Interactive (Full duplex) |
| Audio Input/Output | Mic (Line) Input: On / Off Volume adjustment: Low / Middle / High Audio Output: On / Off Volume adjustment: Low / Middle / High |

|  |  |
| --- | --- |
| OPERATION | |
| Super Dynamic | On / Off The level can be set in the range of 0 to 31. |
| Intelligent Auto | On / Off |
| Adaptive Black Stretch | The level can be set in the range of 0 to 255. |
| Fog compensation | On / Off (only when Intelligent auto / auto contrast adjust: Off) |
| Back light compensation / High light compensation | BLC (Back light compensation) / HLC (High light compensation) / Off (only when Super dynamic / Intelligent Auto: Off) |
| Maximum Gain (AGC) | The level can be set in the range of 0 to 11. |
| Shutter Speed | [60fps mode] 1/60 Fix to 1/10000 Fix  [30fps/15fps mode] 1/30 Fix to 1/10000 Fix  [50fps mode] 1/50 Fix to 1/10000 Fix  [25fps/12.5fps mode] 1/25 Fix to 1/10000 Fix |
| Digital Noise Reduction | The level can be set in the range of 0 to 255. |
| Video Motion Detection (VMD) | On / Off, 4 areas available |
| Scene Change Detection (SCD) | On / Off, 1 area available |
| Privacy Zone | On / Off, Up to 8 zones available |
| Camera Title (OSD) | On / Off, Up to 40 characters (alphanumeric characters, marks) |

|  |  |
| --- | --- |
| BROWSER GUI | |
| Camera Control | Brightness, AUX On / Off |
| GUI/ Setup Menu Language | English, Italian, French, German, Spanish, Portuguese, Russian, Chinese, Japanese |
| Browser | Microsoft Edge, Firefox, Google Chrome |

|  |  |
| --- | --- |
| NETWORK | |
| Network IF | 10Base-T / 100Base-TX, RJ45 connector |
| Supported Protocol   1. IPv6 2. IPv4 | TCP/IP, UDP/IP, HTTP, HTTPS, SSL/TLS, SMTP, DNS, NTP, SNMPv1/v2/v3, DHCPv6,RTP, MLD, ICMP, ARP, IEEE 802.1X,DiffServ, FTP, SFTP, MQTT, LLDP  TCP/IP, UDP/IP, HTTP, HTTPS, SSL/TLS, RTSP, RTP, RTP/RTCP, SMTP, DHCP, DNS, DDNS, NTP, SNMPv1/v2/v3, UPnP, IGMP, ICMP, ARP, IEEE 802.1X, DiffServ, SRTP, FTP, SFTP, MQTT, LLDP |
| No, of Simultaneous Users | Up to 14 users (Depends on network conditions) |
| Secure | FIPS 140-2 level 3 (NXP® EdgeLock® SE050F), Device Certificate GlobalSign® pre-installed, HTTPS, User authentication, Digest authentication, Host authentication, IEEE802.1X, System log, Image transmission log, Brute-force protection, Alteration detection |
| SDXC/SDHC/SD Memory Card   1. H.265 / H.264 recording 2. JPEG recording 3. Compatible SDXC/SDHC/SD Memory Card | Manual REC / Alarm REC (Pre/Post) / Schedule REC / Backup upon network failure  Manual REC / Alarm REC (Pre/Post) / Backup upon network failure   microSDXC memory card: 64 GB, 128 GB, 256 GB, 512 GB microSDHC memory card: 4 GB, 8 GB, 16 GB, 32 GB microSD memory card: 2 GB |
| Mobile Terminal Compatibility | iPad, iPhone, AndroidTM terminals |
| ONVIF® Profile | G / M / S / T |

|  |  |
| --- | --- |
| ALARM | |
| Alarm Source | 3 terminals input, VMD alarm, Command alarm, Audio detection alarm |
| Alarm Actions | SDXC/SDHC/SD memory recording, E-mail notification, HTTP alarm notification Indication on browser, TCP alarm notification output |

|  |  |
| --- | --- |
| INTERFACE | |
| Monitor Output | VBS: 1.0 V [p-p] / 75 Ω, composite, Pin jack  An NTSC or PAL signal can be outputted from camera |
| Microphone input/ Line input | Mic (Line) Input: On / Off Volume adjustment: Low / Middle / High Audio Output: On / Off Volume adjustment: Low / Middle / High |
| Audio Input | ø3.5 mm stereo mini jack For microphone input: Recommended applicable microphone: Plug-in power type  (Sensitivity of microphone: -48 dB±3 dB (0 dB=1 V/Pa, 1 kHz))  Input impedance: Approx. 2 kΩ (unbalanced) Supply voltage: 2.5 V ±0.5 V For line input: Input level: Approx. –10 dBV |
| Audio Output | ø3.5 mm stereo mini jack (monaural output)  Output impedance: Approx. 600 Ω (unbalanced) Output level: –20 dBV |
| External I/O Terminals | ALARM IN 1 (Alarm input 1/ Black & white input/ Auto time adjustment input) (x1)  ALARM IN 2 (Alarm input 2/ ALARM OUT) (x1)  ALARM IN 3 (Alarm input 3/ AUX OUT) (x1) |

|  |  |
| --- | --- |
| ELECTRICAL | |
| Power Source | DC power supply: DC12 V 480 mA, Approx. 5.8 W |
| Power Consumption | PoE (IEEE802.3af compliant) Device: DC48 V 130 mA, Approx. 6.3 W (Class 2 device) |

|  |  |
| --- | --- |
| SAFETY/EMC | |
| Safety | UL (UL62368-1), c-UL (CSA C22.2 No.62368-1), CE, IEC62368-1 |
| EMC | FCC (Part15 ClassA), ICES-003 ClassA, EN55032 ClassB, EN55035 |

|  |  |
| --- | --- |
| MECHANICAL | |
| Dimensions | 75 mm (W) x 57 mm (H) x 146 mm (D) {2-15/16 inches (W) x 2-1/4 inches (H) x 5-3/4 inches (D)}  (excluding lens / power cord plug) |
| Weight | 370 g {0.82 lbs.} |
| Finish   1. Main body 2. Front cover | PC / ABS resin  i-PRO white |

|  |  |
| --- | --- |
| ENVIRONMENTAL | |
| Ambient Operating Temperature | -10 °C to +50 °C (14 °F to 122 °F) |
| Ambient Operating Humidity | 10 to 90 % (no condensation) |