i-PRO WJ-NU301KG NETWORK DISK RECORDER
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 19 DIGITAL VIDEO RECORDERS AND ANALOG RECORDING DEVICES

This specification is intended for use by the design/construction professional and any user of i-PRO Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormatTM 2016 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 
     Warranty | i-PRO Products

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	i-PRO Co., Ltd

B.	Provide Video Surveillance Camera from single source manufacturer 

2.2	i-PRO WJ-NU301KG NETWORK DISK RECORDER

A.	GENERAL CHARACTERISTICS
1.	The Network Disk Recorder (NDR) shall be an all-in-one recording solution for IP video surveillance system of up to 16 network cameras.

2.	The NDR shall store H.264 video data, H.265 video data, and JPEG.

3.	The NDR shall have the capability of up to 256Mbps total throughput. (Recording throughput: 128 Mbps, Output throughput : 128 Mbps)

4.	The NDR shall offer 40TB of gross storage capacity

5.	The NDR shall offer VMD search function which can search the moving of the selected specific area.

6.	The NDR shall record two streams per camera.

　　　　　　　　　　　　　　　　　　　　　　　　
7.	The NDR shall offer displaying videos on the main connected to HDMI interface. 
　
8.	The NDR shall offer the operation and configuration functions to the cameras and NDR from the main monitor connected to HDMI interface and mouse. 

9.	The NDR shall store an encrypted stream and shall display encrypted streams/videos by decrypting.

10.	The NDR shall realize optional SSL / TLS communication with CA certificate. 

11.	The NDR shall offer remote and mobile monitoring on a PC, smartphone and tablet.

12.	The NDR shall conform to the ONVIF standard. 

13.	The NDR shall have 16 PoE ports.

B.	Supported Camera
 1.	Compatible Vendor	i-PRO series Network cameras, 
ONVIF NVT conformant camera and encoder
 2.	Supported Image Format	H.265(HEVC), H.264, JPEG
 3.	Supported Image Resolution
(Depending on the camera)	•Aspect ratio [4 : 3]
 3072x2304, 2560x1920, 2048x1536, 1600x1200, 1280x960, 800x600, 640x480
•Aspect ratio [16 : 9]
 3840x2160, 3328x1872, 3072x1728, 2688x1520, 2560x1440, 1920x1080, 1280x720, 640x360
•Aspect ratio [1 : 1]
 2992x2992, 2816x2816, 2192x2192, 2048x2048, 1440x1440, 1280x1280, 1200x1200
•Aspect ratio [9 : 16]
 2160x3840, 1872x3328, 1728x3072, 1520x2688, 1440x2560, 1080x1920, 720x1280, 360x640
 4.	Supported Audio Format	AAC-LC, G.711 for ONVIF
 5.	Maximum Number of Cameras	MAX. 16

C.	Recording
 1.	Recording Mode	Event, Schedule, Emergency, Pre-event
 2.	Pre-alarm Recording	Up to 15 seconds 
*When the delivery speed from the network camera is less than 4 Mbps.
 3.	Scheduled Recording Mode	4 programs, 6 time zones/day, 
Independent setup for each day of the week
 4.	Frame Rate/Camera	Up to 60 fps
(Depending on the camera)

D.	Main Unit Functions
 1.	Camera Control	Pan/Tilt, Zoom, Focus, Brightness, Preset position call and program (up to 256), Auto mode, Click centering, Wheel zoom, Zoom reset, Auto Back Focus, Aux, Wiper (for WV-SUD638)
 2.	Multiscreen Mode	[Main monitor]
• Control screen 4 / 9/ 16 split screen display
• Wide view screen 2 / 3 / 4 / 5 / 6 / 7 / 9 / 12 / 16 split screen display,1 screen sequence
[Sub monitor]
1 screen sequence, 4 / 9 / 16 split screen display
 3.	Playback Control	PLAY, Rev PLAY, Pause, Stop, FF, FR, Prev Record, Next Record, Prev Image, Next Image, Go to Date, Go to Last (30 s), Time-saving playback
 4.	Search Mode	Search criteria :
Time date, Playback by designating a timeline, VMD, Thumbnail
 5.	Copy	File Format : 
Original Format / MP4
Recorded data of selected cameras and time date range can be copied to USB storage.
 6.	Camera Title	Up to 16 Characters
 7.	Clock Display	Time : 12H/24H
Date : 5 formats
 8.	Digital Zoom	Live / Play: 1.25x 1.5x 1.75x, 2x, 2.5x, 3x, 3.5x 4x, 5x, 6x, 7x, 8x 
(only for 1-screen or 4-screen)
 9.	System Log	Operator access (500), Network error (100), Error (1,000), Event (1000), Operation (500)
 10.	System Setup	Setup page in English, French, Italian, Spanish, German, Portuguese, Thai, Vietnamese, Simplified Chinese, Traditional Chinese, Japanese
 11.	360 Camera Dewarp	Only 1ch display mode.
 12.	re-encoding	2Client
 13.	SD Memory Data Download	Images recorded in the SD card in the i-PRO series cameras can be transferred to the recorder automatically. (H.265/H.264)

E.	Browser GUI
 1.	Camera Control	Pan/Tilt, Zoom, Focus, Brightness, Preset position call and program (up to 256), Auto mode, Zoom reset, Aux, Wiper (for WV-SUD638)
 2.	Playback Control	PLAY, Rev PLAY, Pause, Stop, FF, FR, Prev Record, Next Record, Prev Image, Next Image, Go to Date, Go to Last (30 s)
 3.	Search Mode	Search criteria : 
Time date, Event type, Camera number
 4.	Display Mode	1 screen
 5.	Image Download	File Format : 
Original Format
Recorded data of selected camera and time range can be downloaded to a PC.
Viewer software can be downloaded separately.
 6.	Copy	File Format : 
Original Format / MP4
Recorded data of selected cameras and time date range can be copied to USB storage.
 7.	Camera Title	Up to 16 characters
 8.	Clock Display	On the browser. 
Time: 12H/24H, Date: 5 formats
 9.	Alarm Control	Reset
 10.	System Log	Operator access (500), Network error (100), Error (1,000), Event (1000), Operation (500)
 11.	GUI Language	English, French, Italian, Spanish, German, Portuguese, Thai, Vietnamese, Simplified Chinese, Traditional Chinese, Japanese
 12.	Required PC	CPU: Intel® Core™ i7-860 or faster, 
RAM : 4 GB or more,
VRAM : 128 MB or more (Min. 64 MB), Microsoft® DirectX® 9.0c or later
 13.	Web Browser	Microsoft Edge*, Google Chrome, Mozilla Firefox
*Not compatible with Internet Explorer mode

F.	Alarm/Event
 1.	Alarm Source	4x Terminal inputs, 16x Camera alarms (TCP alarm notification), 128x Command alarms
 2.	Event Mode	Off / On
 3.	Alarm Action	Alarm recording, E-mail notification, Alarm message, Camera positioning, Terminal output, TCP/HTTP alarm notification output, Buzzer, Indicator
 4.	Alarm Control	Reset
 5.	Event log	1000

G.	Input/Output
 1.	Monitor (HDMI) Connector	[Main monitor]
HDMI 4K UHD(3840x2160p)/30Hz, 4K UHD(3840x2160p)/25Hz, 1920x1080p /60Hz, 1920x1080p /50Hz
[Sub monitor] 
HDMI 1920x1080p /60Hz, 1920x1080p /50Hz
 2.	Alarm/Control Terminal	[Alarm] Alarm input 4 , Alarm output 1
[Control]+5 V output, Emergency recording input, General purpose input/output
[Error / Warning] HDD error / Recording error output, Camera error output
 3.	Mouse Connection Port	1 (USB 2.0)
 4.	Network Port (PC)	1x 10BASE-T / 100BASE-TX / 1000BASE-T (RJ45)
 5.	Network Port (Camera)	16x 10BASE-T / 100BASE-TX(RJ45), (RJ45, PoE+),
PoE Budget (16 port Total : Max 233 W, Each port Max : 30 W)
 6.	USB Storage	USB 3.0 / USB 2.0 memory,
USB 3.0 / USB 2.0 connected HDD (except bus powered device)

H.	Network
 1.	Network Interface	10BASE-T / 100BASE-TX / 1000BASE-T (RJ45)
 2.	Maximum Recording Rate	128 Mbps
 3.	Maximum Bandwidth	Total 256 Mbps
 4.	Supported Protocol	IPv4: TCP/IP, UDP/IP, HTTP, HTTPS, SMTP, DNS, NTP, SNMP, RTP, RTSP, ICMP, ARP
IPv6: ICMPv6
 5.	E-mail	Upon Alarm or Warning
 6.	No. of Simultaneous Users	16 or less
 7.	User Registration	Up to 32 users
 8.	User Level	3 Levels (Programmable)
 9.	Partitioning	User level - Camera (View & Control, No Access)
 10.	Security Method	User authentication (ID and Password), Host authentication, Alteration detection, SSL/TLS

I.	Other Functions
 1.	Time Synchronization	NTP (Server/Client)
 2.	Summer Time	User definable (using menu setup)
 3.	Remote Monitoring (Cloud service for P2P)
40 cameras or less
Allows the PC full access to the multiple NU series NVRs.

J.	HDD
 1.	Type	3.5 inch, Max. 2x SATA HDD
 2.	Maximum Capacity	40 TB
 3.	RAID	RAID 1

K.	Viewer Software
 1.	Playback Control	PLAY, Rev PLAY, Pause, FF, FR, Prev Record, Next Record, Prev Image, Next Image
 2.	Additional Functions	[NX Viewer]
Alteration detection, Save as JPEG, Two times zoom, Print, Copy, Aspect ratio switching, fish eye correction, corridor display
 3.	Supported OS, Language	Language of the software will be English or Japanese

L.	General Specifications
 1.	Safety / EMC Standard	DEMKO (IEC62368-1)
CE/UKCA (EN55032/EN55035)
 2.	Power Source	100 - 240 V AC 50 Hz / 60 Hz
 3.	Power Consumption	340W (347 VA)
 4.	Ambient Operating Temperature	Main body : 0 °C to +45 °C (32 °F to 113 °F)
Mouse (provided) : +5 °C to +40 °C (41 °F to 104 °F)
 5.	Ambient Operating Humidity	5 % to 90 % (without condensation)
 6.	Maximum Operating Altitude	2,000 m (6,562 feet) above sea level
 7.	Dimensions	420 mm(W) x 88 mm(H) x 300 mm(D)
{16-17/32 inches (W) x 3-15/32 inches (H) x 11-13/16 inches (D)}
 8.	Mass (approx.)	App 4.7 kg {10.4lbs}