i-PRO WV-S65340-Z4N PTZ NETWORK CAMERA
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SONSORS

This specification is intended for use by the design/construction professional and any user of Panasonic Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormatTM 2016 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 
　  Warranty | i-PRO Products

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	i-PRO Co., Ltd.

B.	Provide Video Surveillance Camera from single source manufacturer 

2.2	i-PRO WV-S65340-Z4N PTZ NETWORK CAMERA

A.	GENERAL CHARACTERISTICS
1.	The PTZ Camera shall deliver H.265 stream and H.264 stream. 

2.	The PTZ Camera shall produce a resolution of 1920 x 1080 pixels(Full HD)
 at up to 60 fps with a 16:9 aspect ratio. 

3.	The PTZ Camera shall produce a resolution of 2048 x 1536 pixels at 15fps with a 4:3 aspect ratio. 

4.	The PTZ Camera shall utilize an approximate 1/2.8-inch type high sensitivity CMOS image sensor.  

5.	The PTZ Camera shall be equipped with 40 times optical zoom. 

6.	The PTZ Camera shall feature an intelligent image stabilization to capture stable images even when installing on the plenty-vibration place. 

7.	The PTZ Camera shall feature a 144dB wide dynamic range based on Enhanced Super Dynamic 

8.	The PTZ Camera shall produce a color image with a minimum illumination of 0.015 lux and a monochrome image with 0.006 lux at F1.6, shutter speed of 1/30s and AGC 11.

9.	The PTZ Camera shall be equipped with a special coated cover for increasing the operational utility of outdoor cameras in rain weather.

10.	The PTZ Camera shall transmit up to four(4) video streams  simultaneously which can be selected to H.265 (Main profile) or H.264 (High profile) or JPEG(can be selected up  to two(2) video streams only).

11.	The PTZ Camera shall be equipped with GOP control of bitrate reducing technology which five control modes included frame rate control for longer recording and less storage.

12.	The PTZ Camera shall produce encrypted stream.

13.	The PTZ Camera shall realize SSL / TLS communication with CA certificate. 

14.	A user shall be able to view video on a PC using a browser.

15.	A user shall be able to view video on a smartphone and tablet using viewer software for iPhone and Android.

16.	The PTZ Camera shall offer Video Motion Detection (VMD) with four (4) programmable detection areas, 15 steps sensitivity level and 10 steps detection size.

17.	The PTZ Camera shall offer intelligent Video Motion Detection (i-VMD) with six (6) detection modes as intruder detection, loitering detection, scene change detection,
object detection and cross line detection

18.	The PTZ Camera shall offer an optional intelligent VMD (i-VMD) function which provides intruder detection, loitering detection, direction detection, scene change detection, object detection and cross line detection.

19.	The PTZ Camera shall have Fog compensation function.

20.	The PTZ Camera shall have High light compensation (HLC) function.

21.	The PTZ Camera shall provide up to thirty-two (32) areas of electronic privacy masking. 

22.	The PTZ Camera shall offer the prioritized stream control which transmits a video stream to a specified client PC or recorder preferentially. 

23.	The PTZ Camera shall have an SD memory card slot that supports SD, SDHC and SDXC memory card for local storage. 

24.	The PTZ Camera shall offer full-duplex bi-directional audio communication capability between the camera and monitoring site. 

25.	The PTZ Camera shall have three (3) alarm sources of terminal input, VMD, command alarm, audio detection alarm and auto track alarm that activate the processes such as SDXC/ SDHC/SD memory recording, E-mail notification, HTTP alarm notification, Indication on browser, FTP image transfer and  TCP alarm notification output.

26.	The PTZ Camera shall conform to the ONVIF profile G / M / S / T and profile. 

B.	Camera
 1.	Image Sensor	Approx. 1/2.8 type CMOS image sensor
 2.	Scanning Area	5.57 mm (H) × 3.13 mm (V)
{7/32 inches (H) × 1/8 inches (V)}
 3.	Minimum Illumination	Color : 0.015 lx (50IRE, F1.6, 1/30s)
Color : 0.001 lx (50IRE, F1.6, 16/30s)
BW : 0.006 lx (50IRE, F1.6, 1/30s)
BW : 0.0004 lx (50IRE, F1.6, 16/30s)
 4.	White Balance	ATW1 / ATW2 / AWC
 5.	Shutter Speed	[60 fps Mode] 1/60 Fix to 1/10000 Fix, 
[30 fps/15 fps mode] 1/30 Fix to 1/10000 Fix 
[50 fps Mode] 1/50 Fix to 1/10000 Fix, 
[25 fps/12.5 fps mode] 1/25 Fix to 1/10000 Fix
 6.	Intelligent Auto	On / Off
 7.	Super Dynamic	On / Off, the level can be set in the range of 0 to 31.
 8.	Dynamic Range	Max.144 dB (Super Dynamic : On, Level 31)
 9.	Adaptive Black Stretch	The level can be set in the range of 0 to 255.
 10.	Back light compensation /
High light compensation	BLC (Back light compensation) / HLC (High light compensation) / Off
The level can be set in the range of 0 to 31 (only when Super dynamic / Intelligent Auto : Off)
 11.	Fog compensation	On / Off, The level can be set in the range of 0 to 8
(only when Intelligent auto / auto contrast adjust : Off)
 12.	Maximum gain (AGC)	The level can be set in the range of 0 to 11.
 13.	Color/BW (ICR)	Off / On / Auto1 / Auto2 / Auto3 (SCC)
 14.	Digital Noise Reduction	The level can be set in the range of 0 to 255.
 15.	Video Motion Detection (VMD)	On / Off, 4 areas available
 16.	Scene Change Detection (SCD)	On / Off, 1 areas available
 17.	Audio Detection	On / Off
 18.	AI Sound Classification	Gunshot, Yell, Vehicle horn, Glass break
 19.	AI Analytics	AI Video Motion Detection, AI Privacy Guard, AI Face Detection, AI People Detection,
AI Vehicle Detection, AI Non mask Detection, AI Occupancy Detection, AI Scene Change Detection

For details :
https://i-pro.com/products_and_solutions/en/surveillance/products/analytics-software
3rd party applications are also available.
https://i-pro.com/products_and_solutions/en/surveillance/solutions/edge-ai-platform/application-list
 20.	Privacy Zone	On / Off, Up to 32 zones available
 21.	VIQS	On / Off, Up to 8 zones available
 22.	Image Stabilizer	On / Off (Built-in gyro sensor)
 23.	Camera Title (OSD)	On / Off, 
Up to 40 characters (alphanumeric characters, marks)
 24.	Focus Adjustment	Auto focus

C.	Lens
 1.	Optical zoom	40x (Motorized zoom / Motorized Focus)
 2.	Extra zoom	Max. 60x (40 to 60x : When resolution is 1280 x 720
 3.	Digital (Electronic) zoom	16x
 4.	Focal Length	4.25 - 170 mm {11/64 inches - 6-11/16 inches}
 5.	Angular Field of View	[16 : 9 mode]
Horizontal : 2.1° (TELE) – 65° (WIDE), Vertical : 1.2° (TELE) – 39° (WIDE)
[ 4 : 3 mode]
Horizontal : 1.6° (TELE) – 51° (WIDE), Vertical : 1.2° (TELE) – 39° (WIDE)
 6.	Maximum Aperture Ratio	1 : 1.6 (WIDE) – 1 : 4.95 (TELE)
 7.	Focus Range	3 m {118-7/64 inches} – ∞

D.	DORI
 1.	Detect (25ppm / 8ppf)	Wide: 60.3m / 197.8 ft, Tele: 2095.2 m / 6873.9 ft
 2.	Observe (62.5ppm / 19ppf)	Wide: 24.1 m / 79.1 ft, Tele: 838.1 m / 2749.5 ft
 3.	Recognize (125ppm / 38ppf)	Wide: 12.1 m / 39.6 ft, Tele: 419.0 m / 1374.8 ft
 4.	Identify (250ppm / 76ppf)	Wide: 6.0m / 19.8 ft, Tele: 209.5 m / 687.4 ft

E.	System on Chip (SoC)
 1.	System on Chip (SoC)	Ambarella CV25M

F.	Adjusting Angle
 1.	Adjusting Angle	Horizontal : 360° Endless Panning, Vertical : -15° to +195°, Yaw : 0°

G.	Pan/tilt
 1.	Panning Range	360° Endless Panning
 2.	Panning Speed	Manual: Approx. 0.065°/s – 150°/s
Preset: Up to approx. 500°/s
 3.	Tilting Range	Operational -15 – +195°
 4.	Tilting Speed	Manual: Approx. 0.065°/s –150°/s Preset: Up to approx. 500°/s
 5.	Preset Positions	256 positions
 6.	Auto Mode	Auto track/ Auto pan/ Preset sequence/ Patrol
 7.	Self Return	10 s/ 20 s/ 30 s/ 1 min/ 2 min/ 3 min/ 5 min/ 10 min/ 20 min/ 30 min/ 60 min

H.	Browser GUI
 1.	Camera Control	Brightness, AUX On / Off
 2.	Audio	Mic (Line) Input : On / Off Volume adjustment : Low / Middle / High
Audio Output : On / Off Volume adjustment : Low / Middle / High
 3.	GUI / Setup Menu Language	English, Italian, French, German, Spanish, Portuguese, Russian, Chinese, Japanese
 4.	Browser	Microsoft Edge, Firefox, Google Chrome

I.	Network
 1.	Network IF	10 Base-T / 100 Base-TX, RJ45 connector
 2.	Resolution H.265/ H.264 JPEG (MJPEG)
[16 : 9 mode (60 fps mode)] , [16 : 9 mode (30 fps mode)],
[16 : 9 mode (50 fps mode)] , [16 : 9 mode (25 fps mode)]
1920x1080, 1280x720, 640x360, 320x180
[4 : 3 mode (30 fps mode)], [4 : 3 mode (25 fps mode)]
1280x960, VGA, QVGA
[4 : 3 mode (15 fps mode)], [4 : 3 mode (12.5 fps mode)]
2048x1536 , 1280x960, VGA, QVGA
 3.	H.265/H.264	[Transmission Mode]
Constant bit rate / VBR / Frame rate / Best effort
[Transmission Type]
Unicast port (AUTO) / Unicast port (MANUAL) / Multicast
 4.	JPEG	[Image Quality]
10 steps
 5.	Smart Coding	GOP (Group of pictures) control:
 Off/ Low (Variable GOP 1s-8s)/ Mid (Variable GOP 4s-16s)/ 
 Advanced(Fixed GOP 60s w/1s key-frame)/
 Frame rate control (Variable GOP 4s-16s with frame rate control)
 *Advanced and Frame rate control are only available with H.265.
Smart VIQS: On(High)/On(Low)/Off, Smart P-picture control: On/Off
 6.	Audio Compression	G.726 (ADPCM) : 16 kbps / 32 kbps 
G.711 : 64 kbps
AAC-LC : 64 kbps / 96 kbps / 128 kbps
 7.	Audio Transmission Mode	Off / Mic (Line) input / Audio output / Interactive (Half duplex) / Interactive (Full duplex)
 8.	Supported Protocol	IPv6 : TCP/IP, UDP/IP, HTTP, HTTPS, SSL/TLS, SMTP, DNS, NTP, SNMPv1/v2/v3, 
 DHCPv6, RTP, MLD, ICMP, ARP, IEEE 802.1X, DiffServ, SFTP, MQTT, LLDP
IPv4 : TCP/IP, UDP/IP, HTTP, HTTPS, SSL/TLS, RTSP, RTP, RTP/RTCP, SMTP, 
 DHCP, DNS, DDNS, NTP, SNMPv1/v2/v3, UPnP, IGMP, ICMP, ARP, 
 IEEE 802.1X, DiffServ, SRTP, SFTP, MQTT, LLDP, NTCIP
 9.	No. of Simultaneous Users	Up to 14 users (Depends on network conditions)
 10.	Secure	FIPS 140-2 level 3 (NXP® EdgeLock® SE050F), Device Certificate GlobalSign® pre-installed,
HTTPS, User authentication, Digest authentication, Host authentication,
IEEE802.1X, System log, Image transmission log, Brute-force protection, Alteration detection, Signed Firmware (V2.50 or later)
 11.	SDXC/SDHC/SD Memory Card (Option)	H.265 / H.264 recording :
 Manual REC / Alarm REC (Pre/Post) / Schedule REC / Backup upon network failure
JPEG recording :
 Manual REC / Alarm REC (Pre/Post) / Backup upon network failure 
Compatible SDXC/SDHC/SD Memory Card :
 microSDXC memory card : 64 GB, 128 GB, 256 GB, 512 GB
 microSDHC memory card : 4 GB, 8 GB, 16 GB, 32 GB 
 microSD memory card : 2 GB
 12.	Mobile Terminal Compatibility	iPad, iPhone (iOS 8.0 or later), Android™ terminals
 13.	ONVIF® Profile	G / M / S / T

J.	Alarm
 1.	Alarm Source	3 terminals input, VMD alarm, Command alarm, Audio detection alarm
 2.	Alarm Actions	SDXC/SDHC/SD memory recording, E-mail notification, 
HTTP alarm notification Indication on browser, TCP alarm notification output

K.	Input/Output
 1.	Audio Input	ø3.5 mm stereo mini jack 
For microphone input : Recommended applicable microphone : Plug-in power type 
(Sensitivity of microphone : –51 dB to –38 dB (0 dB=1 V/Pa, 1 kHz)) 
Input impedance : Approx. 2 kΩ (unbalanced)
Supply voltage : 2.5 V ±0.5 V

For line input : Input level : Approx. –10 dBV
 2.	Audio Output	ø3.5 mm stereo mini jack (monaural output) 
Output impedance : Approx. 600 Ω (unbalanced) 
Output level : –20 dBV
 3.	External I/O Terminals	ALARM IN 1 (Alarm input 1/ Black & white input/ Auto time adjustment input) (x1)
ALARM IN 2 (Alarm input 2/ ALARM OUT) (x1), ALARM IN 3 (Alarm input 3/ AUX OUT) (x1)
 4.	Monitor Output	Yes (for adjustment)
Φ3.5mm stereo mini jack, NTSC or PAL signal can be output from camera

L.	General
 1.	Safety	UL (UL62368-1), c-UL (CSA C22.2 No.62368-1), CE, IEC62368-1
 2.	EMC	FCC (Part15 ClassA), ICES-003 Issue 7 ClassA, EN55032 ClassA, EN55035
 3.	Power Source and Power Consumption	AC24 V, PoE++ (IEEE802.3bt),PoE+ (IEEE802.3at)
AC24 V, 3.4 A Approx. 53.3 W
PoE++ DC 54 V 940 mA, Approx. 50.84 W(Class6 device)
PoE+ DC 54 V 470 mA, Approx. 25.4 W(Class4 device)
 4.	Ambient Operating Temperature	-50 °C to +60 °C (-58 °F to +140 °F)
(AC24V, PoE++)
-30 °C to +60°C {-22 °F to +140 °F)(PoE+ device)
(Power On range : –30 °C to +60 °C {–22 °F to +140 °F})
Maximum temperature according to NEMA TS2(2.2.7) : 74 °C(165 °F)
 5.	Ambient Operating Humidity	10 to 100 % (no condensation)
 6.	Anti-Condensation System	Temish element + Heater + FAN + ROSAHL
 7.	Water and Dust Resistance	IP66, IP67, IEC60529 measuring standard compatible, Type 4X(UL50E), NEMA 4X compliant
 8.	Shock Resistance	IK10 (IEC 62262)
 9.	Wind Resistance	Up to 40 m/s {approx. 89 mph}
 10.	Other standard support	NEMA TS2(2.2.7-2.2.9)
 11.	Dimensions	ø229 mm x 278 mm (H) {ø9-1/32 inches x 10-15/16 inches (H)}
 12.	Mass (Approx.)	Approx. 4.3 kg {9.48 lbs.}
 13.	Finish	Main body : Aluminum die cast, i-PRO white
Outer fixing screws : Stainless steel (Corrosion-resistant treatment)
Dome section : Polycarbonate resin, Clear (with ClearSight coating)