13.4.1 Configure settings relating to image quality on alarm action
Click “Image compression rate upon alarm detection” of “Camera action on alarm” on the [Alarm] tab of the “Alarm” page. (→13.4 Configure the settings relating to the camera action on alarm occurrence [Alarm])
[Image compression rate upon alarm detection]
Select “On” or “Off” to determine whether or not to change the image quality of “Quality1” (→11.2 Configure the settings relating to JPEG images [JPEG/H.264]) upon alarm detection.
•
On: Images will be transmitted with the image quality selected for “Image quality upon alarm detection”.
•
Off: Does not change the image quality upon alarm detection.
•
Default: Off
[Image quality upon alarm detection]
Image quality can be changed upon an alarm occurrence. Select the image quality from the following.
0 Super fine/ 1 Fine/ 2/ 3/ 4/ 5 Normal/ 6/ 7/ 8/ 9 Low
•
Default: 5 Normal