Section 7 Playback of images on the SD memory card
When clicking a time and date listed on the log list window, the “Live” page will turn to the “Playback” page.
When images associated with the clicked time and date are on the SD memory card, the first image of them will be displayed.
The display format varies depending on the “Recording format” of the SD memory card.
IMPORTANT
•
Refresh interval of images may become slow during playback or download.
•
When many images are saved on the SD memory card, it may take time to display images on the “Playback” page.
•
Images will be displayed in VGA size on the “Playback” page regardless of the image capture size of the images saved on the SD memory card. When the aspect ratio is “16:9”, images will be displayed in “640x360” on the “Playback” page regardless of the image capture size of the images saved on the SD memory card. Therefore, images may look coarse on the “Playback” page.
•
When playing images by selecting an FTP error log on the log list, images may not be played in order of images recorded on the SD memory card if they have been recorded on the SD memory card with selected value for the “Transmission interval” setting of “FTP periodic image transmission” on the [Advanced] tab is “1min” or less.
•
The playback refresh interval may become slower when recording data to the SD memory card.