Section 17 Configure the settings relating to the schedules [Schedule]
On the “Schedule” page, it is possible to configure the settings relating to schedules as follows.
•
VMD permission
•
Access permission
•
H.264 recording
•
Scene file
•
FTP periodic image transmission
The “Schedule” page has only the [Schedule] tab.
Up to 5 schedules can be set.
1.
Select an action to be assigned to the schedule from “Schedule mode”.
“Off” is selected at the default.
•
Off: No action will be taken for the respective schedule.
•
VMD permission: The video motion detection (VMD) function will be active during the period of the schedule.
•
Access permission: Users whose access level is set to 2 and 3 on the [User auth.] tab (→15.1 Configure the settings relating to the user authentication [User auth.]) can access the camera only in the period of schedule.
•
H.264 recording(Recording stream 1): The SD recording will be performed at the designated time in the schedule. Only available when H.264 images are used.
•
H.264 recording(Recording stream 2): The SD recording will be performed at the designated time in the schedule. Only available when H.264 images are used.
•
Image adjust 1: Images are set to the image settings of “Scene file 1” at the designated time in the schedule. When the designated time for the schedule finishes, images are set to the image settings of “Scene file is not applied”.
•
Image adjust 2: Images are set to the image settings of “Scene file 2” at the designated time in the schedule. When the designated time for the schedule finishes, images are set to the image settings of “Scene file is not applied”.
•
FTP periodic image transmission: FTP periodic image transmission will be performed at the designated time in the schedule.
Note
•
Select “On” for “User auth.” on the [User auth.] tab of “User mng.” page (→15.1 Configure the settings relating to the user authentication [User auth.]) and “Off” for “Host auth.” on the “Host auth.” page (→15.2 Configure the settings relating to the host authentication [Host auth.]) to validate “Access permission”.
•
When selecting “H.264 recording(Recording stream 1)” or “H.264 recording(Recording stream 2)”, select “H.264(1)”, “H.264(2)”, “H.264(3)”, or “H.264(4)” for “Recording format” on the [SD memory card] tab and select “Schedule” for “Save trigger”. (→10.3 Configure the settings relating to the SD memory card [SD memory card])
2.
Select days of a week by checking the respective checkboxes.
3.
From the pull-down menu, select the start time and the end time of the schedule.
When not designating time, check the checkbox of “24h”.
4.
Click the [Set] button after completing the settings.
→
The result will be displayed at the bottom of the window.
Note
•
The schedules displayed at the bottom of the window can be identified by colors assigned to each schedule.