10.6 Access copy images saved on the SD memory card onto the PC [SD memory card images]
Click the [SD memory card] tab on the “Basic” page. (→9.1 How to display the setup menu, 9.2 How to operate the setup menu)
The following are descriptions of how to copy images saved on the SD memory card onto the PC. It is necessary in advance to select “Allow” for “FTP access to camera” on the [Network] tab of the “Network” page. (→16.1 Configure the network settings [Network])
IMPORTANT
•
It may sometimes be impossible to operate when another user is accessing images on the SD memory card. In this case, retry later.
•
Depending on the settings of a proxy server or a firewall, images may not be obtained via a network. In this case, refer to the network administrator.
1.
Click the [Execute] button.
→
The user authentication window will be displayed.
2.
Click the [OK] button after entering the user name and password of the camera administrator.
→
The folder in which images are to be saved will be displayed.
Note
•
When the FTP server of the camera is logged to access images, the SD memory card is assigned to Drive B.
Images are saved in different directories according to “Save trigger”.
Move to the directory corresponding to the desired images and copy them.
Refer to Section 22 Directory structure of drive B for further information about the directory structure.
Possible number of JPEG images that can be saved on the SD memory card (as indications)
For the possible number of JPEG images that can be saved on the SD memory card, refer to our website below.
http://security.panasonic.com/pss/security/support/info.html
Possible duration of H.264 images that can be saved on the SD memory card (as indications)
For possible duration of H.264 images that can be saved on the SD memory card, refer to our website below.
http://security.panasonic.com/pss/security/support/info.html